| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
WALLILIM
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

WALLILIM Bit Field. More...

## Macros
#define | LTC4155_WALLILIM_SUBADDR LTC4155_REG1_SUBADDR
| WALLILIM More...
#define | LTC4155_WALLILIM_SIZE 5
#define | LTC4155_WALLILIM_OFFSET 0
#define | LTC4155_WALLILIM_MASK 0x1F
#define | LTC4155_WALLILIM (LTC4155_WALLILIM_OFFSET << 12 | (LTC4155_WALLILIM_SIZE - 1) << 8 | LTC4155_WALLILIM_SUBADDR)
#define | LTC4155_WALLILIM_PRESET__100MA 0x0
#define | LTC4155_WALLILIM_PRESET__500MA 0x1
#define | LTC4155_WALLILIM_PRESET__600MA 0x2
#define | LTC4155_WALLILIM_PRESET__700MA 0x3
#define | LTC4155_WALLILIM_PRESET__800MA 0x4
#define | LTC4155_WALLILIM_PRESET__900MA 0x5
#define | LTC4155_WALLILIM_PRESET__1P00A 0x6
#define | LTC4155_WALLILIM_PRESET__1P25A 0x7
#define | LTC4155_WALLILIM_PRESET__1P50A 0x8
#define | LTC4155_WALLILIM_PRESET__1P75A 0x9
#define | LTC4155_WALLILIM_PRESET__2P00A 0xA
#define | LTC4155_WALLILIM_PRESET__2P25A 0xB
#define | LTC4155_WALLILIM_PRESET__2P50A 0xC
#define | LTC4155_WALLILIM_PRESET__2P75A 0xD
#define | LTC4155_WALLILIM_PRESET__3P00A 0xE
#define | LTC4155_WALLILIM_PRESET__2P5MA_SUSPEND 0xF
#define | LTC4155_WALLILIM_PRESET_CLPROG_1 0x1F

## Detailed Description

WALLILIM Bit Field.

WALL total input current limit setting. Register contents will be modified by the LTC4155 upon certain events. See the datasheet section Input Current Regulation.

- Register: REG1
- CommandCode: 0x01
- Size: 5
- Offset: 0
- MSB: 4
- MASK: 0x1F
- Access: R/W
- Default: n/a

## Macro Definition Documentation

## ◆ LTC4155_WALLILIM

#define LTC4155_WALLILIM (LTC4155_WALLILIM_OFFSET << 12 | (LTC4155_WALLILIM_SIZE - 1) << 8 | LTC4155_WALLILIM_SUBADDR)

Definition at line 286 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_MASK

#define LTC4155_WALLILIM_MASK 0x1F

Definition at line 285 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_OFFSET

#define LTC4155_WALLILIM_OFFSET 0

Definition at line 284 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__100MA

#define LTC4155_WALLILIM_PRESET__100MA 0x0

Definition at line 287 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__1P00A

#define LTC4155_WALLILIM_PRESET__1P00A 0x6

Definition at line 293 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__1P25A

#define LTC4155_WALLILIM_PRESET__1P25A 0x7

Definition at line 294 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__1P50A

#define LTC4155_WALLILIM_PRESET__1P50A 0x8

Definition at line 295 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__1P75A

#define LTC4155_WALLILIM_PRESET__1P75A 0x9

Definition at line 296 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__2P00A

#define LTC4155_WALLILIM_PRESET__2P00A 0xA

Definition at line 297 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__2P25A

#define LTC4155_WALLILIM_PRESET__2P25A 0xB

Definition at line 298 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__2P50A

#define LTC4155_WALLILIM_PRESET__2P50A 0xC

Definition at line 299 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__2P5MA_SUSPEND

#define LTC4155_WALLILIM_PRESET__2P5MA_SUSPEND 0xF

Definition at line 302 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__2P75A

#define LTC4155_WALLILIM_PRESET__2P75A 0xD

Definition at line 300 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__3P00A

#define LTC4155_WALLILIM_PRESET__3P00A 0xE

Definition at line 301 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__500MA

#define LTC4155_WALLILIM_PRESET__500MA 0x1

Definition at line 288 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__600MA

#define LTC4155_WALLILIM_PRESET__600MA 0x2

Definition at line 289 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__700MA

#define LTC4155_WALLILIM_PRESET__700MA 0x3

Definition at line 290 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__800MA

#define LTC4155_WALLILIM_PRESET__800MA 0x4

Definition at line 291 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET__900MA

#define LTC4155_WALLILIM_PRESET__900MA 0x5

Definition at line 292 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_PRESET_CLPROG_1

#define LTC4155_WALLILIM_PRESET_CLPROG_1 0x1F

Definition at line 303 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_SIZE

#define LTC4155_WALLILIM_SIZE 5

Definition at line 283 of file LTC4155_reg_defs.h.

## ◆ LTC4155_WALLILIM_SUBADDR

#define LTC4155_WALLILIM_SUBADDR LTC4155_REG1_SUBADDR

WALLILIM

Definition at line 282 of file LTC4155_reg_defs.h.