| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Files
LTC2947 a high-precision power and energy monitor with an internal sense resistor supporting up to 30A.
Power Monitors and Coulomb Counters

LTC2947: LTC2947 a high-precision power and energy monitor with an internal sense resistor supporting up to 30A. More...

## Files
file | LTC2947.cpp
| Library for LTC2947: A high-precision power and energy monitor with an internal sense resistor supporting up to 30A.
file | LTC2947.h
| LTC2947: LTC2947 a high-precision power and energy monitor with an internal sense resistor supporting up to 30A.
file | DC2334A.ino
file | DC2574A_KIT.ino
| Linduino.INO File for DC2574A_KIT: Standalone power/energy monitor for evaluation of the LTC2947 monitor without a PC Linear Technology DC2574A_KIT Demonstration Board: Standalone power/energy monitor for evaluation of the LTC2947 monitor without a PC. LTC2947: high-precision power and energy monitor with an internal sense resistor supporting up to 30A.

## Detailed Description

LTC2947: LTC2947 a high-precision power and energy monitor with an internal sense resistor supporting up to 30A.

    The LTC2947 is a high-precision power and energy
    monitor with an internal sense resistor supporting up
    to 30A. Three internal No Latency delta sigma ADCs ensure
    accurate measurement of voltage and current, while high-
    bandwidth analog multiplication of voltage and current
    provides accurate power measurement in a wide range of
    applications. Internal or external clocking options enable
    precise charge and energy measurements.
    An internal 300 micro ohms, temperature-compensated sense
    resistor minimizes efficiency loss and external compo-
    nents, simplifying energy measurement applications while
    enabling high accuracy current measurement over the full
    temperature range. For more details see following URLs:

http://www.linear.com/product/LTC2947

http://www.linear.com/product/LTC2947#demoboards

Copyright 2018(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.