| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions
LTC2752.cpp File Reference
Digital-to-Analog Converters (DAC) » LTC2752: Dual Serial 16-Bit SoftSpan IOUT DAC

Library for LTC2752 Dual Serial 16-Bit SoftSpan IOUT DAC. More...

## Detailed Description

Library for LTC2752 Dual Serial 16-Bit SoftSpan IOUT DAC.

Definition in file LTC2752.cpp.

Go to the source code of this file.

## Functions
void | LTC2752_write (uint8_t cs, uint8_t dac_command, uint8_t dac_address, uint16_t data)
| Transmits 24 bit input stream: 4-bit command + 4-bit don't-care + 16-bit data. More...
float | LTC2752_code_to_voltage (uint16_t dac_code, float min_output, float max_output)
| Calculate the LTC2752 DAC output voltage given the DAC code and and the minimum / maximum outputs for a given softspan range. More...
uint16_t | LTC2752_voltage_to_code (float dac_voltage, float min_output, float max_output)
| Calculate a LTC2752 DAC code given the desired output voltage and the minimum / maximum outputs for a given softspan range. More...

## Function Documentation

## ◆ LTC2752_code_to_voltage()

float LTC2752_code_to_voltage | ( | uint16_t | dac_code,
|  | float | min_output,
|  | float | max_output
| ) |  |

Calculate the LTC2752 DAC output voltage given the DAC code and and the minimum / maximum outputs for a given softspan range.

Returns
  Floating point voltage

Definition at line 87 of file LTC2752.cpp.

## ◆ LTC2752_voltage_to_code()

uint16_t LTC2752_voltage_to_code | ( | float | dac_voltage,
|  | float | min_output,
|  | float | max_output
| ) |  |

Calculate a LTC2752 DAC code given the desired output voltage and the minimum / maximum outputs for a given softspan range.

Returns
  16 bit data

Definition at line 96 of file LTC2752.cpp.

## ◆ LTC2752_write()

void LTC2752_write | ( | uint8_t | cs,
|  | uint8_t | dac_command,
|  | uint8_t | dac_address,
|  | uint16_t | data
| ) |  |

Transmits 24 bit input stream: 4-bit command + 4-bit don't-care + 16-bit data.

Returns
  void

Definition at line 77 of file LTC2752.cpp.