| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Files
LTC6813-1: Multicell Battery Monitor
Battery Management System (BMS)

LTC6813: Multicell Battery Monitors. More...

## Files
file | LTC6813.cpp
| Library for LTC6813-1 Multicell Battery Monitor.
file | LTC6813.h
| LTC6813: Multicell Battery Monitors.
file | DC2350AB.ino
| Analog Devices DC2350A-B Demonstration Board.

## Detailed Description

LTC6813: Multicell Battery Monitors.

    *The LTC6813 is multi-cell battery stack monitor that measures up to 18 series
    *connected battery cells with a total measurement error of less than 2.2mV.
    *The cell measurement range of 0V to 5V makes the LTC6813 suitable for most
    *battery chemistries. All 18 cell voltages can be captured in 290uS, and lower
    *data acquisition rates can be selected for high noise reduction.
    *Using the LTC6813-1, multiple devices are connected in a daisy-chain with one
    *host processor connection for all devices, permitting simultaneous cell monitoring
    *of long, high voltage battery strings.
    *

https://www.analog.com/en/products/ltc6813-1.html https://www.analog.com/en/design-center/evaluation-hardware-and-software/evaluation-boards-kits/dc2350a-b.html

Copyright 2019(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.