| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Files
LTC2607: 16-Bit, Dual Rail-to-Rail DACs with I2C Interface
Digital-to-Analog Converters (DAC)

LTC2607: 16-Bit, Dual Rail-to-Rail DACs with I2C Interface. More...

## Files
file | LTC2607.cpp
| Library for LTC2607: 16-Bit, Dual Rail-to-Rail DACs with I2C Interface.
file | LTC2607.h
| LTC2607: 16-Bit, Dual Rail-to-Rail DACs with I2C Interface.
file | DC934A.ino
| Linear Technology DC934 Demonstration Board.
file | FAE_April_2013.ino
| DC934A Science Project FAE Meeting April 2013.

## Detailed Description

LTC2607: 16-Bit, Dual Rail-to-Rail DACs with I2C Interface.

LTC2609: Quad 16-/14-/12-Bit Rail-to-Rail DACs with I²C Interface. LTC2606: 16-Bit Rail-to-Rail DACs with I²C Interface.

    The LTC2607/LTC2617/LTC2627 are dual 16-, 14- and 12-bit, 2.7V to 5.5V
    rail-to-rail voltage output DACs in a 12-lead DFN package. They have built-in
    high performance output buffers and are guaranteed monotonic.

    These parts establish new board-density benchmarks for 16- and 14-bit DACs and
    advance performance standards for output drive and load regulation in single-
    supply, voltage-output DACs.

    The parts use a 2-wire, I2C compatible serial interface. The
    LTC2607/LTC2617/LTC2627 operate in both the standard mode (clock rate of 100kHz)
    and the fast mode (clock rate of 400kHz). An asynchronous DAC update pin (LDAC)
    is also included.

    The LTC2607/LTC2617/LTC2627 incorporate a power-on reset circuit. During power-
    up, the voltage outputs rise less than 10mV above zero scale; and after power-
    up, they stay at zero scale until a valid write and update take place. The
    power-on reset circuit resets the LTC2607-1/LTC2617-1/ LTC2627-1 to mid-scale.
    The voltage outputs stay at midscale until a valid write and update takes place.

http://www.linear.com/product/LTC2607 http://www.linear.com/product/LTC2609 http://www.linear.com/product/LTC2606

http://www.linear.com/product/LTC2607#demoboards http://www.linear.com/product/LTC2609#demoboards http://www.linear.com/product/LTC2606#demoboards

Copyright 2018(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.