| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Files
LTC3589: 8-Output Regulator with Sequencing and I2C
Switching Regulators, Battery Chargers, and LED Drivers

LTC3589: 8-Output Regulator with Sequencing and I2C. More...

## Files
file | LTC3589.cpp
| Library for LTC3589: 8-Output Regulator with Sequencing and I2C.
file | LTC3589.h
| LTC3589: 8-Output Regulator with Sequencing and I2C.
file | DC1558_DC1808.ino
| Linear Technology DC1558 and DC1808 Demonstration Boards.

## Detailed Description

LTC3589: 8-Output Regulator with Sequencing and I2C.

    The LTC3589 is a complete power management solution for ARM and ARM-based
    processors and advanced portable microprocessor systems. The device contains
    three step-down DC/DC converters for core, memory and SoC rails, a
    buck-boost regulator for I/O at 1.8V to 5V and three 250mA LDO regulators
    for low noise analog supplies. An I2C serial port is used to control enables,
    output voltage levels, dynamic voltage scaling, operating modes and status
    reporting.
    Regulator start-up is sequenced by connecting outputs to enable pins in the
    desired order or programmed via the I2C port. System power-on, power-off,
    and reset functions are controlled by pushbutton interface, pin inputs, or
    I2C interface.
    The LTC3589 supports i.MX53/51, PXA and OMAP processors with eight
    independent rails at appropriate power levels. Other features include
    interface signals such as the VSTB pin that simultaneously toggle up to
    four rails between programmed run and standby output voltages.  The device
    is available in a low profile 40-pin 6mm x 6mm exposed pad QFN package.

    I2C DATA FORMAT (MSB FIRST)

http://www.linear.com/product/LTC3589

http://www.linear.com/product/LTC3589#demoboards

Copyright 2018(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.