| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
TIMER
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

TIMER Bit Field. More...

## Macros
#define | LTC4155_TIMER_SUBADDR LTC4155_REG1_SUBADDR
| TIMER More...
#define | LTC4155_TIMER_SIZE 2
#define | LTC4155_TIMER_OFFSET 5
#define | LTC4155_TIMER_MASK 0x60
#define | LTC4155_TIMER (LTC4155_TIMER_OFFSET << 12 | (LTC4155_TIMER_SIZE - 1) << 8 | LTC4155_TIMER_SUBADDR)
#define | LTC4155_TIMER_PRESET__4_HOUR 0x0
#define | LTC4155_TIMER_PRESET__8_HOUR_OR_COVERX 0x1
#define | LTC4155_TIMER_PRESET__1_HOUR 0x2
#define | LTC4155_TIMER_PRESET__2_HOUR 0x3

## Detailed Description

TIMER Bit Field.

User Programmed Li-Ion charger safety timer setting. This internal timer begins at the onset of constant-voltage charging. Charging terminates at the expiration of the selected time.

- Register: REG1
- CommandCode: 0x01
- Size: 2
- Offset: 5
- MSB: 6
- MASK: 0x60
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_TIMER

#define LTC4155_TIMER (LTC4155_TIMER_OFFSET << 12 | (LTC4155_TIMER_SIZE - 1) << 8 | LTC4155_TIMER_SUBADDR)

Definition at line 261 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_MASK

#define LTC4155_TIMER_MASK 0x60

Definition at line 260 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_OFFSET

#define LTC4155_TIMER_OFFSET 5

Definition at line 259 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_PRESET__1_HOUR

#define LTC4155_TIMER_PRESET__1_HOUR 0x2

Definition at line 264 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_PRESET__2_HOUR

#define LTC4155_TIMER_PRESET__2_HOUR 0x3

Definition at line 265 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_PRESET__4_HOUR

#define LTC4155_TIMER_PRESET__4_HOUR 0x0

Definition at line 262 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_PRESET__8_HOUR_OR_COVERX

#define LTC4155_TIMER_PRESET__8_HOUR_OR_COVERX 0x1

Definition at line 263 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_SIZE

#define LTC4155_TIMER_SIZE 2

Definition at line 258 of file LTC4155_reg_defs.h.

## ◆ LTC4155_TIMER_SUBADDR

#define LTC4155_TIMER_SUBADDR LTC4155_REG1_SUBADDR

TIMER

Definition at line 257 of file LTC4155_reg_defs.h.