| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions
LTC2366.cpp File Reference
Analog-to-Digital Converters (ADC) » LTC2366: 12-Bit 3Msps ADC

Library for LTC2366: 12-Bit 3Msps ADC. More...

## Detailed Description

Library for LTC2366: 12-Bit 3Msps ADC.

Definition in file LTC2366.cpp.

Go to the source code of this file.

## Functions
void | LTC2366_read (uint8_t cs, uint16_t *ptr_adc_code)
| Reads the LTC2366 and returns 32-bit data in offset binary format. More...
float | LTC2366_code_to_voltage (uint16_t adc_code, float vref)
| Calculates the LTC2366 input voltage given the binary data and lsb weight. More...

## Function Documentation

## ◆ LTC2366_code_to_voltage()

float LTC2366_code_to_voltage | ( | uint16_t | adc_code,
|  | float | vref
| ) |  |

Calculates the LTC2366 input voltage given the binary data and lsb weight.

Returns
  Floating point voltage

Parameters

  adc_code | Raw ADC code
  vref | Reference voltage

Definition at line 97 of file LTC2366.cpp.

## ◆ LTC2366_read()

void LTC2366_read | ( | uint8_t | cs,
|  | uint16_t * | ptr_adc_code
| ) |  |

Reads the LTC2366 and returns 32-bit data in offset binary format.

Returns
  void

Parameters

  cs | Chip Select Pin
  ptr_adc_code | Returns code read from ADC (from previous conversion)

Definition at line 85 of file LTC2366.cpp.