| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Files
LTC6952: Ultralow Jitter, 4.5GHz PLL with 11 Outputs and JESD204B Support
RF, Silicon Oscillators, PLL Synthesizers, and VCOs

LTC6952: Ultralow Jitter, 4.5GHz PLL with 11 Outputs and JESD204B Support. More...

## Files
file | LTC6952.cpp
| Library for LTC6952: Ultralow Jitter, 4.5GHz PLL with 11 Outputs and JESD204B Support.
file | LTC6952.h
| LTC6952: Ultralow Jitter, 4.5GHz PLL with 11 Outputs and JESD204B Support.
file | DC2609A.ino
| DC2609A LTC6952: Ultralow Jitter, 4.5GHz PLL with 11 Outputs and JESD204B Support.

## Detailed Description

LTC6952: Ultralow Jitter, 4.5GHz PLL with 11 Outputs and JESD204B Support.

    The LTC®6952 is a high performance, ultralow jitter,
    JESD204B clock generation and distribution IC. It includes
    a Phase Locked Loop (PLL) core, consisting of a reference
    divider, phase-frequency detector (PFD) with a phase-lock
    indicator, ultralow noise charge pump and integer feedback
    divider. The LTC6952’s eleven outputs can be configured
    as up to five JESD204B subclass 1 device clock/SYSREF
    pairs plus one general purpose output, or simply eleven
    general purpose clock outputs for non-JESD204B applications.
    Each output has its own individually programmable
    frequency divider and output driver. All outputs can also
    be synchronized and set to precise phase alignment using
    individual coarse half-cycle digital delays and fine analog
    time delays.
    For applications requiring more than eleven total outputs,
    multiple LTC6952s can be connected together using the
    EZSync or ParallelSync synchronization protocols.

http://www.linear.com/product/LTC6952

http://www.linear.com/product/LTC6952#demoboards

Copyright 2018(c) Analog Devices, Inc.

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

- Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
- Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
- Neither the name of Analog Devices, Inc. nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.
- The use of this software may or may not infringe the patent rights of one or more patent holders. This license does not release you from the requirement that you obtain separate licenses from these patent holders to use this software.
- Use of the software either in source or binary form, must be run on or directly connected to an Analog Devices Inc. component.

THIS SOFTWARE IS PROVIDED BY ANALOG DEVICES "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, NON-INFRINGEMENT, MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL ANALOG DEVICES BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, INTELLECTUAL PROPERTY RIGHTS, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.