| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

MasterAddressConstants.h
Go to the documentation of this file.
1 //EEPROM functions take 8-bit address, which is inconsistent with all other code
2 #define I2C_Board0_EEPROM_ADDR0 (0x51<<1)
3 #define I2C_Board0_LTC2485_Iout_LH_ADDR0 0x15
4 #define I2C_Board0_LTC2485_Iout_LH_Global 0x76
5 #define I2C_Board0_LTC2485_Vout_LF_ADDR0 0x14
6 #define I2C_Board0_LTC2485_Vout_LF_Global 0x76
7 #define I2C_Board0_LTC2655_LLL_ADDR0 0x11
8 #define I2C_Board0_LTC2655_LLL_Global 0x72
9 #define I2C_Board1_EEPROM_ADDR0 (0x59<<1)
10 #define I2C_Board1_LTC2485_Iout_LH_ADDR0 0x1D
11 #define I2C_Board1_LTC2485_Iout_LH_Global 0x7E
12 #define I2C_Board1_LTC2485_Vout_LF_ADDR0 0x1C
13 #define I2C_Board1_LTC2485_Vout_LF_Global 0x7E
14 #define I2C_Board1_LTC2655_LLL_ADDR0 0x19
15 #define I2C_Board1_LTC2655_LLL_Global 0x7A
16 #define I2C_Board2_EEPROM_ADDR0 (0x41<<1)
17 #define I2C_Board2_LTC2485_Iout_LH_ADDR0 0x05
18 #define I2C_Board2_LTC2485_Iout_LH_Global 0x66
19 #define I2C_Board2_LTC2485_Vout_LF_ADDR0 0x04
20 #define I2C_Board2_LTC2485_Vout_LF_Global 0x66
21 #define I2C_Board2_LTC2655_LLL_ADDR0 0x01
22 #define I2C_Board2_LTC2655_LLL_Global 0x62
23 #define I2C_Board3_EEPROM_ADDR0 (0x49<<1)
24 #define I2C_Board3_LTC2485_Iout_LH_ADDR0 0x0D
25 #define I2C_Board3_LTC2485_Iout_LH_Global 0x6E
26 #define I2C_Board3_LTC2485_Vout_LF_ADDR0 0x0C
27 #define I2C_Board3_LTC2485_Vout_LF_Global 0x6E
28 #define I2C_Board3_LTC2655_LLL_ADDR0 0x09
29 #define I2C_Board3_LTC2655_LLL_Global 0x6A
30 #define I2C_Board4_EEPROM_ADDR0 (0x71<<1)
31 #define I2C_Board4_LTC2485_Iout_LH_ADDR0 0x35
32 #define I2C_Board4_LTC2485_Iout_LH_Global 0x56
33 #define I2C_Board4_LTC2485_Vout_LF_ADDR0 0x34
34 #define I2C_Board4_LTC2485_Vout_LF_Global 0x56
35 #define I2C_Board4_LTC2655_LLL_ADDR0 0x31
36 #define I2C_Board4_LTC2655_LLL_Global 0x52
37 #define I2C_Board5_EEPROM_ADDR0 (0x79<<1)
38 #define I2C_Board5_LTC2485_Iout_LH_ADDR0 0x3D
39 #define I2C_Board5_LTC2485_Iout_LH_Global 0x5E
40 #define I2C_Board5_LTC2485_Vout_LF_ADDR0 0x3C
41 #define I2C_Board5_LTC2485_Vout_LF_Global 0x5E
42 #define I2C_Board5_LTC2655_LLL_ADDR0 0x39
43 #define I2C_Board5_LTC2655_LLL_Global 0x5A
44 #define I2C_Board6_EEPROM_ADDR0 (0x61<<1)
45 #define I2C_Board6_LTC2485_Iout_LH_ADDR0 0x25
46 #define I2C_Board6_LTC2485_Iout_LH_Global 0x46
47 #define I2C_Board6_LTC2485_Vout_LF_ADDR0 0x24
48 #define I2C_Board6_LTC2485_Vout_LF_Global 0x46
49 #define I2C_Board6_LTC2655_LLL_ADDR0 0x21
50 #define I2C_Board6_LTC2655_LLL_Global 0x42
51 #define I2C_Board7_EEPROM_ADDR0 (0x69<<1)
52 #define I2C_Board7_LTC2485_Iout_LH_ADDR0 0x2D
53 #define I2C_Board7_LTC2485_Iout_LH_Global 0x4E
54 #define I2C_Board7_LTC2485_Vout_LF_ADDR0 0x2C
55 #define I2C_Board7_LTC2485_Vout_LF_Global 0x4E
56 #define I2C_Board7_LTC2655_LLL_ADDR0 0x29
57 #define I2C_Board7_LTC2655_LLL_Global 0x4A
58 //!touchscreen I2C address
59 #define I2C_FT6206_ADDR0 0x38