| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Macros
CXSET
Switching Regulators, Battery Chargers, and LED Drivers » LTC4155: Dual-Input Power Manager / 3.5A Li-Ion Battery Charger with I²C Control and USB OTG » LTC4155 Register Map Definitions

CXSET Bit Field. More...

## Macros
#define | LTC4155_CXSET_SUBADDR LTC4155_REG2_SUBADDR
| CXSET More...
#define | LTC4155_CXSET_SIZE 2
#define | LTC4155_CXSET_OFFSET 0
#define | LTC4155_CXSET_MASK 0x03
#define | LTC4155_CXSET (LTC4155_CXSET_OFFSET << 12 | (LTC4155_CXSET_SIZE - 1) << 8 | LTC4155_CXSET_SUBADDR)
#define | LTC4155_CXSET_PRESET__10PCT 0x0
#define | LTC4155_CXSET_PRESET__20PCT 0x1
#define | LTC4155_CXSET_PRESET__2PCT 0x2
#define | LTC4155_CXSET_PRESET__5PCT 0x3

## Detailed Description

CXSET Bit Field.

End-of-Charge indication current threshold setting. This threshold can also be used for charge termination if TIMER is set to 8_Hour_or_CoverX.

- Register: REG2
- CommandCode: 0x02
- Size: 2
- Offset: 0
- MSB: 1
- MASK: 0x03
- Access: R/W
- Default: 0

## Macro Definition Documentation

## ◆ LTC4155_CXSET

#define LTC4155_CXSET (LTC4155_CXSET_OFFSET << 12 | (LTC4155_CXSET_SIZE - 1) << 8 | LTC4155_CXSET_SUBADDR)

Definition at line 406 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_MASK

#define LTC4155_CXSET_MASK 0x03

Definition at line 405 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_OFFSET

#define LTC4155_CXSET_OFFSET 0

Definition at line 404 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_PRESET__10PCT

#define LTC4155_CXSET_PRESET__10PCT 0x0

Definition at line 407 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_PRESET__20PCT

#define LTC4155_CXSET_PRESET__20PCT 0x1

Definition at line 408 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_PRESET__2PCT

#define LTC4155_CXSET_PRESET__2PCT 0x2

Definition at line 409 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_PRESET__5PCT

#define LTC4155_CXSET_PRESET__5PCT 0x3

Definition at line 410 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_SIZE

#define LTC4155_CXSET_SIZE 2

Definition at line 403 of file LTC4155_reg_defs.h.

## ◆ LTC4155_CXSET_SUBADDR

#define LTC4155_CXSET_SUBADDR LTC4155_REG2_SUBADDR

CXSET

Definition at line 402 of file LTC4155_reg_defs.h.