| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Data Structures | Macros
Adafruit_ILI9341.h File Reference

Go to the source code of this file.

## Data Structures
class | Adafruit_ILI9341

## Macros
#define | ILI9341_TFTWIDTH 240
#define | ILI9341_TFTHEIGHT 320
#define | ILI9341_NOP 0x00
#define | ILI9341_SWRESET 0x01
#define | ILI9341_RDDID 0x04
#define | ILI9341_RDDST 0x09
#define | ILI9341_SLPIN 0x10
#define | ILI9341_SLPOUT 0x11
#define | ILI9341_PTLON 0x12
#define | ILI9341_NORON 0x13
#define | ILI9341_RDMODE 0x0A
#define | ILI9341_RDMADCTL 0x0B
#define | ILI9341_RDPIXFMT 0x0C
#define | ILI9341_RDIMGFMT 0x0D
#define | ILI9341_RDSELFDIAG 0x0F
#define | ILI9341_INVOFF 0x20
#define | ILI9341_INVON 0x21
#define | ILI9341_GAMMASET 0x26
#define | ILI9341_DISPOFF 0x28
#define | ILI9341_DISPON 0x29
#define | ILI9341_CASET 0x2A
#define | ILI9341_PASET 0x2B
#define | ILI9341_RAMWR 0x2C
#define | ILI9341_RAMRD 0x2E
#define | ILI9341_PTLAR 0x30
#define | ILI9341_MADCTL 0x36
#define | ILI9341_PIXFMT 0x3A
#define | ILI9341_FRMCTR1 0xB1
#define | ILI9341_FRMCTR2 0xB2
#define | ILI9341_FRMCTR3 0xB3
#define | ILI9341_INVCTR 0xB4
#define | ILI9341_DFUNCTR 0xB6
#define | ILI9341_PWCTR1 0xC0
#define | ILI9341_PWCTR2 0xC1
#define | ILI9341_PWCTR3 0xC2
#define | ILI9341_PWCTR4 0xC3
#define | ILI9341_PWCTR5 0xC4
#define | ILI9341_VMCTR1 0xC5
#define | ILI9341_VMCTR2 0xC7
#define | ILI9341_RDID1 0xDA
#define | ILI9341_RDID2 0xDB
#define | ILI9341_RDID3 0xDC
#define | ILI9341_RDID4 0xDD
#define | ILI9341_GMCTRP1 0xE0
#define | ILI9341_GMCTRN1 0xE1
#define | ILI9341_BLACK 0x0000 /* 0, 0, 0 */
#define | ILI9341_NAVY 0x000F /* 0, 0, 128 */
#define | ILI9341_DARKGREEN 0x03E0 /* 0, 128, 0 */
#define | ILI9341_DARKCYAN 0x03EF /* 0, 128, 128 */
#define | ILI9341_MAROON 0x7800 /* 128, 0, 0 */
#define | ILI9341_PURPLE 0x780F /* 128, 0, 128 */
#define | ILI9341_OLIVE 0x7BE0 /* 128, 128, 0 */
#define | ILI9341_LIGHTGREY 0xC618 /* 192, 192, 192 */
#define | ILI9341_DARKGREY 0x7BEF /* 128, 128, 128 */
#define | ILI9341_BLUE 0x001F /* 0, 0, 255 */
#define | ILI9341_GREEN 0x07E0 /* 0, 255, 0 */
#define | ILI9341_CYAN 0x07FF /* 0, 255, 255 */
#define | ILI9341_RED 0xF800 /* 255, 0, 0 */
#define | ILI9341_MAGENTA 0xF81F /* 255, 0, 255 */
#define | ILI9341_YELLOW 0xFFE0 /* 255, 255, 0 */
#define | ILI9341_WHITE 0xFFFF /* 255, 255, 255 */
#define | ILI9341_ORANGE 0xFD20 /* 255, 165, 0 */
#define | ILI9341_GREENYELLOW 0xAFE5 /* 173, 255, 47 */
#define | ILI9341_PINK 0xF81F

## Macro Definition Documentation

## ◆ ILI9341_BLACK

#define ILI9341_BLACK 0x0000 /* 0, 0, 0 */

Definition at line 98 of file Adafruit_ILI9341.h.

## ◆ ILI9341_BLUE

#define ILI9341_BLUE 0x001F /* 0, 0, 255 */

Definition at line 107 of file Adafruit_ILI9341.h.

## ◆ ILI9341_CASET

#define ILI9341_CASET 0x2A

Definition at line 62 of file Adafruit_ILI9341.h.

## ◆ ILI9341_CYAN

#define ILI9341_CYAN 0x07FF /* 0, 255, 255 */

Definition at line 109 of file Adafruit_ILI9341.h.

## ◆ ILI9341_DARKCYAN

#define ILI9341_DARKCYAN 0x03EF /* 0, 128, 128 */

Definition at line 101 of file Adafruit_ILI9341.h.

## ◆ ILI9341_DARKGREEN

#define ILI9341_DARKGREEN 0x03E0 /* 0, 128, 0 */

Definition at line 100 of file Adafruit_ILI9341.h.

## ◆ ILI9341_DARKGREY

#define ILI9341_DARKGREY 0x7BEF /* 128, 128, 128 */

Definition at line 106 of file Adafruit_ILI9341.h.

## ◆ ILI9341_DFUNCTR

#define ILI9341_DFUNCTR 0xB6

Definition at line 75 of file Adafruit_ILI9341.h.

## ◆ ILI9341_DISPOFF

#define ILI9341_DISPOFF 0x28

Definition at line 59 of file Adafruit_ILI9341.h.

## ◆ ILI9341_DISPON

#define ILI9341_DISPON 0x29

Definition at line 60 of file Adafruit_ILI9341.h.

## ◆ ILI9341_FRMCTR1

#define ILI9341_FRMCTR1 0xB1

Definition at line 71 of file Adafruit_ILI9341.h.

## ◆ ILI9341_FRMCTR2

#define ILI9341_FRMCTR2 0xB2

Definition at line 72 of file Adafruit_ILI9341.h.

## ◆ ILI9341_FRMCTR3

#define ILI9341_FRMCTR3 0xB3

Definition at line 73 of file Adafruit_ILI9341.h.

## ◆ ILI9341_GAMMASET

#define ILI9341_GAMMASET 0x26

Definition at line 58 of file Adafruit_ILI9341.h.

## ◆ ILI9341_GMCTRN1

#define ILI9341_GMCTRN1 0xE1

Definition at line 91 of file Adafruit_ILI9341.h.

## ◆ ILI9341_GMCTRP1

#define ILI9341_GMCTRP1 0xE0

Definition at line 90 of file Adafruit_ILI9341.h.

## ◆ ILI9341_GREEN

#define ILI9341_GREEN 0x07E0 /* 0, 255, 0 */

Definition at line 108 of file Adafruit_ILI9341.h.

## ◆ ILI9341_GREENYELLOW

#define ILI9341_GREENYELLOW 0xAFE5 /* 173, 255, 47 */

Definition at line 115 of file Adafruit_ILI9341.h.

## ◆ ILI9341_INVCTR

#define ILI9341_INVCTR 0xB4

Definition at line 74 of file Adafruit_ILI9341.h.

## ◆ ILI9341_INVOFF

#define ILI9341_INVOFF 0x20

Definition at line 56 of file Adafruit_ILI9341.h.

## ◆ ILI9341_INVON

#define ILI9341_INVON 0x21

Definition at line 57 of file Adafruit_ILI9341.h.

## ◆ ILI9341_LIGHTGREY

#define ILI9341_LIGHTGREY 0xC618 /* 192, 192, 192 */

Definition at line 105 of file Adafruit_ILI9341.h.

## ◆ ILI9341_MADCTL

#define ILI9341_MADCTL 0x36

Definition at line 68 of file Adafruit_ILI9341.h.

## ◆ ILI9341_MAGENTA

#define ILI9341_MAGENTA 0xF81F /* 255, 0, 255 */

Definition at line 111 of file Adafruit_ILI9341.h.

## ◆ ILI9341_MAROON

#define ILI9341_MAROON 0x7800 /* 128, 0, 0 */

Definition at line 102 of file Adafruit_ILI9341.h.

## ◆ ILI9341_NAVY

#define ILI9341_NAVY 0x000F /* 0, 0, 128 */

Definition at line 99 of file Adafruit_ILI9341.h.

## ◆ ILI9341_NOP

#define ILI9341_NOP 0x00

Definition at line 40 of file Adafruit_ILI9341.h.

## ◆ ILI9341_NORON

#define ILI9341_NORON 0x13

Definition at line 48 of file Adafruit_ILI9341.h.

## ◆ ILI9341_OLIVE

#define ILI9341_OLIVE 0x7BE0 /* 128, 128, 0 */

Definition at line 104 of file Adafruit_ILI9341.h.

## ◆ ILI9341_ORANGE

#define ILI9341_ORANGE 0xFD20 /* 255, 165, 0 */

Definition at line 114 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PASET

#define ILI9341_PASET 0x2B

Definition at line 63 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PINK

#define ILI9341_PINK 0xF81F

Definition at line 116 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PIXFMT

#define ILI9341_PIXFMT 0x3A

Definition at line 69 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PTLAR

#define ILI9341_PTLAR 0x30

Definition at line 67 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PTLON

#define ILI9341_PTLON 0x12

Definition at line 47 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PURPLE

#define ILI9341_PURPLE 0x780F /* 128, 0, 128 */

Definition at line 103 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PWCTR1

#define ILI9341_PWCTR1 0xC0

Definition at line 77 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PWCTR2

#define ILI9341_PWCTR2 0xC1

Definition at line 78 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PWCTR3

#define ILI9341_PWCTR3 0xC2

Definition at line 79 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PWCTR4

#define ILI9341_PWCTR4 0xC3

Definition at line 80 of file Adafruit_ILI9341.h.

## ◆ ILI9341_PWCTR5

#define ILI9341_PWCTR5 0xC4

Definition at line 81 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RAMRD

#define ILI9341_RAMRD 0x2E

Definition at line 65 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RAMWR

#define ILI9341_RAMWR 0x2C

Definition at line 64 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDDID

#define ILI9341_RDDID 0x04

Definition at line 42 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDDST

#define ILI9341_RDDST 0x09

Definition at line 43 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDID1

#define ILI9341_RDID1 0xDA

Definition at line 85 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDID2

#define ILI9341_RDID2 0xDB

Definition at line 86 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDID3

#define ILI9341_RDID3 0xDC

Definition at line 87 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDID4

#define ILI9341_RDID4 0xDD

Definition at line 88 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDIMGFMT

#define ILI9341_RDIMGFMT 0x0D

Definition at line 53 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDMADCTL

#define ILI9341_RDMADCTL 0x0B

Definition at line 51 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDMODE

#define ILI9341_RDMODE 0x0A

Definition at line 50 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDPIXFMT

#define ILI9341_RDPIXFMT 0x0C

Definition at line 52 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RDSELFDIAG

#define ILI9341_RDSELFDIAG 0x0F

Definition at line 54 of file Adafruit_ILI9341.h.

## ◆ ILI9341_RED

#define ILI9341_RED 0xF800 /* 255, 0, 0 */

Definition at line 110 of file Adafruit_ILI9341.h.

## ◆ ILI9341_SLPIN

#define ILI9341_SLPIN 0x10

Definition at line 45 of file Adafruit_ILI9341.h.

## ◆ ILI9341_SLPOUT

#define ILI9341_SLPOUT 0x11

Definition at line 46 of file Adafruit_ILI9341.h.

## ◆ ILI9341_SWRESET

#define ILI9341_SWRESET 0x01

Definition at line 41 of file Adafruit_ILI9341.h.

## ◆ ILI9341_TFTHEIGHT

#define ILI9341_TFTHEIGHT 320

Definition at line 38 of file Adafruit_ILI9341.h.

## ◆ ILI9341_TFTWIDTH

#define ILI9341_TFTWIDTH 240

Definition at line 37 of file Adafruit_ILI9341.h.

## ◆ ILI9341_VMCTR1

#define ILI9341_VMCTR1 0xC5

Definition at line 82 of file Adafruit_ILI9341.h.

## ◆ ILI9341_VMCTR2

#define ILI9341_VMCTR2 0xC7

Definition at line 83 of file Adafruit_ILI9341.h.

## ◆ ILI9341_WHITE

#define ILI9341_WHITE 0xFFFF /* 255, 255, 255 */

Definition at line 113 of file Adafruit_ILI9341.h.

## ◆ ILI9341_YELLOW

#define ILI9341_YELLOW 0xFFE0 /* 255, 255, 0 */

Definition at line 112 of file Adafruit_ILI9341.h.