| Linduino 1.3.0 Linear Technology Arduino-Compatible Demonstration Board

Functions
LTC2460.cpp File Reference
Analog-to-Digital Converters (ADC) » LTC2460: 24-Bit, 16-Channel Delta Sigma ADCs with Selectable Speed/Resolution

Library for LTC2460: 24-Bit, 16-Channel Delta Sigma ADCs with Selectable Speed/Resolution. More...

## Detailed Description

Library for LTC2460: 24-Bit, 16-Channel Delta Sigma ADCs with Selectable Speed/Resolution.

Definition in file LTC2460.cpp.

Go to the source code of this file.

## Functions
void | LTC2460_read (uint8_t cs, uint8_t adc_command, int32_t *adc_code)
float | LTC2460_code_to_voltage (int32_t adc_code, float vref)
| Calculates the voltage corresponding to an adc code, given the reference (in volts) More...

## Function Documentation

## ◆ LTC2460_code_to_voltage()

float LTC2460_code_to_voltage | ( | int32_t | adc_code,
|  | float | vref
| ) |  |

Calculates the voltage corresponding to an adc code, given the reference (in volts)

Returns
  Returns voltage calculated from ADC code.

Parameters

  adc_code | Code read from adc
  vref | VRef (in volts)

Definition at line 86 of file LTC2460.cpp.

## ◆ LTC2460_read()

void LTC2460_read | ( | uint8_t | cs,
|  | uint8_t | adc_command,
|  | int32_t * | adc_code
| ) |  |

Reads from LTC2460.

Parameters

  cs | Chip select
  adc_command | 1 byte command written to LTC2460
  adc_code | 4 byte conversion code read from LTC2460

Definition at line 77 of file LTC2460.cpp.