ARMWSD Downloader | Context

The ARMWSD downloader can be started with or without a command line option. If it is started with the full name of a *.ini file it will use this file to store its parameters. Alternatively parameters are stored in armwsd.ini in the same folder as the ARMWSD.exe file.

The ARMWSD loader main screen is shown below:

.

To download a program proceed as follows:

- Connect your hardware to an available COM port of your computer using a suitable RS232 cable.
- Start the ARMWSD software.
- If necessary click the Configure key and set the required communications options.
- If necessary select the File to Download using the Browse button.
- Click on the Start button.
- On the hardware hold down the Download switch and press the reset switch. The selected data will be downloaded.
- Press the Run button to run the program.
- Note the Monitor Status box which gives helpful hints.