<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN">
<HTML>
<HEAD>
	<TITLE>ArmDownloader</title>
	<LINK REL="STYLESHEET" HREF="..\AIDEB.css" TYPE="text/css">
</HEAD>
<BODY>
<TABLE BORDER=0 Cellpading=2 WIDTH="100%">
<TR>
	<TD CLASS="S"><B><FONT SIZE="5">
		<A HREF="AD_P.html" TARGET="_parent">ARMWSD Downloader
		</A></FONT SIZE></B>
	<TD CLASS="X">
		<A HREF="AD_P.html" TARGET="_parent">
		<img SRC="..\Context_I.png" BORDER=0>Context</A>
</TR>
</TABLE>
<P>
The ARMWSD downloader can be started with or without a command line option. 
If it is started with the full name of a *.ini file it will use this file
to store its parameters. Alternatively parameters are stored in armwsd.ini 
in the same folder as the ARMWSD.exe file.<P>

The ARMWSD loader main screen is shown below:<P>
<img SRC="AD.png" BORDER=0>.<P>

To download a program proceed as follows:<P>

<UL>
	<LI>Connect your hardware to an available COM port of your computer
	using a suitable RS232 cable.
	<LI>Start the ARMWSD software.
	<LI>If necessary click the <A HREF="ADC_B.html">Configure</A> key and set 
	the required communications options.
	<LI>If necessary select the <B>File to Download</B> using the 
	<B>Browse</B> button.
	<LI>Click on the <B>Start</B> button.
	<LI>On the hardware hold down the Download switch and press the reset 
	switch. The selected data will be downloaded.
	<LI>Press the <B>Run</B> button to run the program.
	<LI>Note the <B>Monitor Status</B> box which gives helpful hints.
</UL>
			<HR WIDTH="80%">
</BODY>
</HTML>




