<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN">
<HTML>
<HEAD>
	<TITLE>ArmDownloaderConfigBody</title>
	<LINK REL="STYLESHEET" HREF="AIDEB.css" TYPE="text/css">
</HEAD>
<BODY>
<TABLE BORDER=0 Cellpading=2 WIDTH="100%">
<TR>
	<TD CLASS="S"><B><FONT SIZE="5">
		<A HREF="AD_P.html" TARGET="_parent">ARMWSD Configuration
		</A></FONT SIZE></B>
	<TD CLASS="X">
		<A HREF="AD_P.html" TARGET="_parent">
		<img SRC="Context_I.png" BORDER=0>Context</A>
</TR>
</TABLE>
<P>
The configuration screen allows the user to configure the <B>Help</B>, 
<B>Communications</B> details, <B>Flash</B> actions and <B>Protection</B> 
options and an example is shown below.<P>

<img SRC="ADCH.png" BORDER=0>.<P>

<H3>Communications</H3>

Choose the desired RS232 <B>Serial Port</B> and <B>Baudrate</B>.<P>

<H3>Flash</H3>

Choose whether you want the part to be fully erased (<B>Mass Erase</B>) or only 
the necessary parts erased before each programming.<P>

Select the <B>Program</B> option unless you just want to erase teh part.<P>

Select the <B>Verify</B> option if you want the program verified after 
programming.<P>

<H3>Help</H3>

In the <B>Browser</B> edit box type the full path and application name of the
browser you would like to use for help.<P>

In the <B>Help Path</B> edit box type the full path to the help files. If you do 
not know where they are search for AD_B.html and use its path.<P>

<H3>Exit</H3>

Press the <B>OK</B> button to fix these settings or <B>Cancel</B> to discard the 
changes.<P>

			<HR WIDTH="80%">
</BODY>
</HTML>




