Altium Designer Pick and Place Locations
C:\Users\Kasutaja\Desktop\SYSTEEM\MEGA\PCB_PROJECTS\Trinamic\4BreakoutBoards\TMC4671\V1_1\Outputs\FABRICATION\Pick Place\TMC4671-BOB_V1.1.txt

========================================================================================================================
File Design Information:

Date:       05.10.17
Time:       19:17
Revision:   Not in VersionControl
Variant:    All fitted
Units used: mil

Designator Comment                            Layer    Footprint                Center-X(mil) Center-Y(mil) Rotation Description                                                                                    
R400       1k                                 TopLayer R0603                    506.535       1549.998      180      1 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series                                       
R401       1k                                 TopLayer R0603                    502.360       1450.998      180      1 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series                                       
D401       LED, Blue, SMD, 20mA, 2.8V, 465 nm TopLayer LED_0603                 382.360       1450.998      180      LED, Blue, SMD, 20mA, 2.8V, 465 nm                                                             
D400       LED, Blue, SMD, 20mA, 2.8V, 465 nm TopLayer LED_0603                 386.535       1549.998      180      LED, Blue, SMD, 20mA, 2.8V, 465 nm                                                             
XTL100     25MHz                              TopLayer FOX924B-25.000           895.798       1395.065      360      TCXO, 25 MHz, 2.5 ppm, SMD, 5mm x 3.2mm, HCMOS, 3.3 V, FOX924 Series                           
TVS201     SRV05-4.TCT                        TopLayer SOT95P280X145-6N         1257.401      510.000       90       ESD Protection Device, TVS, 17.5 V, SOT-23, 6 Pins, 5 V, 300 W                                 
TVS200     SRV05-4.TCT                        TopLayer SOT95P280X145-6N         1257.401      210.000       90       ESD Protection Device, TVS, 17.5 V, SOT-23, 6 Pins, 5 V, 300 W                                 
R311       100k                               TopLayer R0603                    1366.379      1391.892      90       SMD Chip Resistor, Thick Film, 100 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series   
R310       1k5                                TopLayer R0603                    1092.677      1388.108      90       SMD Chip Resistor, Thick Film, 1.5 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series   
R309       100R                               TopLayer R0603                    305.864       181.287       180      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series    
R308       100R                               TopLayer R0603                    306.067       421.467       180      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series    
R307       10k                                TopLayer R0603                    467.207       485.843       360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series       
R306       10k                                TopLayer R0603                    467.207       421.800       180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series       
R305       10k                                TopLayer R0603                    465.864       178.200       360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series       
R304       10k                                TopLayer R0603                    465.864       114.157       180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series       
R211       4k7                                TopLayer R0603                    1151.000      411.465       270      SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series               
R210       4k7                                TopLayer R0603                    1151.000      104.465       270      SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series               
R209       4k7                                TopLayer R0603                    1151.000      533.000       90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series               
R208       4k7                                TopLayer R0603                    1151.000      226.000       90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series               
R207       4k7                                TopLayer R0603                    956.000       612.000       90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series               
R206       4k7                                TopLayer R0603                    956.000       312.000       90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series               
R205       22R                                TopLayer R0603                    1360.000      510.000       270      SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
R204       22R                                TopLayer R0603                    1330.000      400.000       360      SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
R203       22R                                TopLayer R0603                    1330.000      340.000       360      SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
R202       22R                                TopLayer R0603                    1360.000      210.000       270      SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
R201       22R                                TopLayer R0603                    1330.000      100.000       360      SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
R200       22R                                TopLayer R0603                    1330.000      40.000        360      SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
R101       1k2                                TopLayer R0603                    265.000       655.000       270      SMD Chip Resistor, Thick Film, 1.2 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series   
R100       10k                                TopLayer R0603                    986.586       966.414       45       SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series       
P103       DF20F-10DP-1V(56)                  TopLayer CON,_TMC_Debug_SPI       479.094       1225.748      180      Wire-To-Board Connector, 1 mm, 10 Contacts, Header, DF20 Series, Surface Mount, 2 Rows         
L100       30R                                TopLayer L0603                    683.490       1397.425      90       Ferrite Bead, 30 ohm, 0603 [1608 Metric], MFB Series, 3 A, 0.04 ohm, ± 25%                     
IC201      SN74LVC3G17DCUR                    TopLayer TSSOP50P310X90-8L        975.945       497.945       180      Triple Schmitt-Trigger Buffer, 74LVC3G17, 1.65 V to 5.5 V, VSSOP-8                             
IC200      SN74LVC3G17DCUR                    TopLayer TSSOP50P310X90-8L        975.945       190.945       180      Triple Schmitt-Trigger Buffer, 74LVC3G17, 1.65 V to 5.5 V, VSSOP-8                             
IC100      TMC4671                            TopLayer QFN40P1050X650X90_HS-77N 635.117       810.982       360                                                                                                     
D300       BAT54S                             TopLayer SOT95P237X130-3N         1261.772      1390.000      360      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                    
D102       BAT54S                             TopLayer SOT95P237X130-3N         183.228       1264.998      180      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                    
D101       BAT54S                             TopLayer SOT95P237X130-3N         183.228       1134.998      180      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                    
D100       LTST-C191KRKT                      TopLayer LED_0603                 318.000       618.535       270      Green 631nm LED Indication - Discrete 2V 0603 (1608 Metric)                                    
C411       4u7                                TopLayer C0603                    578.053       585.000       90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 4.7 µF, 10 V, ± 10%, X5R, MC Series      
C410       470nF                              TopLayer C0603                    848.465       1052.998      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.47 µF, 16 V, ± 10%, X5R, MC Series     
C409       100nF                              TopLayer C0603                    848.465       993.000       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C408       47uF/10V                           TopLayer C1206                    950.000       1180.000      270      SMD Multilayer Ceramic Capacitor, 1206 [3216 Metric], 47 µF, 10 V, ± 20%, X5R, GRM Series      
C407       100nF/10V                          TopLayer C0603                    960.000       755.000       180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C406       100nF/10V                          TopLayer C0603                    677.000       1046.000      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C405       100nF/10V                          TopLayer C0603                    960.000       815.000       180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C404       100nF/10V                          TopLayer C0603                    532.000       1016.496      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C403       100nF/10V                          TopLayer C0603                    430.000       605.000       90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C402       100nF/10V                          TopLayer C0603                    385.000       935.000       270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C401       100nF/10V                          TopLayer C0603                    619.000       1016.496      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C400       100nF/10V                          TopLayer C0603                    369.999       674.998       90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C302       10nF                               TopLayer C0603                    1156.732      1388.108      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.01 µF, 10 V, ± 10%, X7R, MCSH Series   
C301       100pF/50V/5%                       TopLayer C0603                    305.864       117.243       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C300       100pF/50V/5%                       TopLayer C0603                    306.067       486.467       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C209       100nF/10V                          TopLayer C0603                    956.000       414.945       180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C208       100nF/10V                          TopLayer C0603                    956.000       107.945       180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C207       100pF/50V/5%                       TopLayer C0603                    1093.000      411.465       90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C206       100pF/50V/5%                       TopLayer C0603                    1093.000      104.465       90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C205       100pF/50V/5%                       TopLayer C0603                    1093.000      533.000       270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C204       100pF/50V/5%                       TopLayer C0603                    1093.000      226.000       270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C203       100pF/50V/5%                       TopLayer C0603                    1014.000      611.000       270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C202       100pF/50V/5%                       TopLayer C0603                    1014.000      311.000       270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series 
C201       100nF/10V                          TopLayer C0603                    1208.535      628.465       180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C200       100nF/10V                          TopLayer C0603                    1209.000      317.000       180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
C100       100nF/10V                          TopLayer C0603                    742.545       1397.425      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series      
R300       0R                                 TopLayer R0603                    683.490       1207.559      270      SMD Chip Resistor, Thick Film, 0 ohm, 0603 [1608 Metric], 100 mW, MCWR Series                  
R301       0R                                 TopLayer R0603                    742.545       1207.559      90       SMD Chip Resistor, Thick Film, 0 ohm, 0603 [1608 Metric], 100 mW, MCWR Series                  
R302       0R                                 TopLayer R0603                    801.601       1207.559      270      SMD Chip Resistor, Thick Film, 0 ohm, 0603 [1608 Metric], 100 mW, MCWR Series                  
R303       0R                                 TopLayer R0603                    860.656       1207.559      90       SMD Chip Resistor, Thick Film, 0 ohm, 0603 [1608 Metric], 100 mW, MCWR Series                  
