Altium Designer Pick and Place Locations
C:\Users\Kasutaja\Desktop\SYSTEEM\MEGA\PCB_PROJECTS\Trinamic\TMC_EVAL_boards\TMC4671_EVAL\V1_1\Outputs\FABRICATION\Pick Place\TMC4671-EVAL_V1.1.txt

========================================================================================================================
File Design Information:

Date:       04.05.18
Time:       21:11
Revision:   Not in VersionControl
Variant:    Variant of TMC4671-EVAL_V1_0
Units used: mil

Designator Comment            Layer       Footprint                Center-X(mil) Center-Y(mil) Rotation Description                                                                                      
IC200      TMC4671            TopLayer    QFN40P1050X650X90_HS-77N 1082.677      1686.500      90                                                                                                        
R509       1k5                TopLayer    R0603                    1549.685      693.040       180      SMD Chip Resistor, Thick Film, 1.5 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
D502       BAT54S             TopLayer    SOT95P237X130-3N         1154.015      850.686       360      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
D501       BAT54S             TopLayer    SOT95P237X130-3N         1285.905      850.686       360      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
D500       BAT54S             TopLayer    SOT95P237X130-3N         1417.795      850.686       360      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
TVS303     SRV05-4.TCT        TopLayer    SOT95P280X145-6N         716.142       3027.166      180      ESD Protection Device, TVS, 17.5 V, SOT-23, 6 Pins, 5 V, 300 W                                   
TVS302     SRV05-4.TCT        TopLayer    SOT95P280X145-6N         1208.268      3027.166      180      ESD Protection Device, TVS, 17.5 V, SOT-23, 6 Pins, 5 V, 300 W                                   
TVS301     SRV05-4.TCT        TopLayer    SOT95P280X145-6N         708.268       2615.355      180      ESD Protection Device, TVS, 17.5 V, SOT-23, 6 Pins, 5 V, 300 W                                   
TVS300     SRV05-4.TCT        TopLayer    SOT95P280X145-6N         1208.268      2615.355      180      ESD Protection Device, TVS, 17.5 V, SOT-23, 6 Pins, 5 V, 300 W                                   
R504       100R               TopLayer    R0603                    1154.015      693.040       180      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series      
R503       100R               TopLayer    R0603                    1285.906      693.040       180      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series      
R502       100R               TopLayer    R0603                    1417.795      693.040       180      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series      
R501       100R               TopLayer    R0603                    1437.166      1500.002      360      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series      
R407       10k                TopLayer    R0603                    1437.165      1618.110      360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R406       10R                BottomLayer R0603                    1782.676      437.059       90       SMD Chip Resistor, Thick Film, 10 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R403       10k                TopLayer    R0603                    1437.165      1913.386      180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R404       10k                TopLayer    R0603                    1437.166      1736.220      360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R401       10k                TopLayer    R0603                    1437.166      2031.495      180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R402       10k                TopLayer    R0603                    1437.165      1854.331      360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R400       10k                TopLayer    R0603                    1437.166      1972.440      360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R323       4k7                BottomLayer R0603                    1035.040      3117.717      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R322       4k7                BottomLayer R0603                    1535.040      3117.717      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R321       4k7                BottomLayer R0603                    1035.040      2705.906      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R320       4k7                BottomLayer R0603                    1535.040      2705.906      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R319       4k7                BottomLayer R0603                    901.180       3117.717      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R318       4k7                BottomLayer R0603                    1401.180      3117.717      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R317       4k7                BottomLayer R0603                    901.180       2705.906      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R316       4k7                BottomLayer R0603                    1401.180      2705.906      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R315       4k7                BottomLayer R0603                    767.322       3117.717      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R314       4k7                BottomLayer R0603                    1267.322      3117.717      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R313       4k7                BottomLayer R0603                    767.322       2705.906      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R312       4k7                BottomLayer R0603                    1267.322      2705.906      90       SMD Chip Resistor, 4.7 kohm, 75 V, 0603 [1608 Metric], 100 mW, ± 1%, WR06 Series                 
R311       22R                BottomLayer R0603                    822.440       3117.717      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R310       22R                BottomLayer R0603                    956.300       3117.717      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R309       22R                BottomLayer R0603                    1090.158      3117.717      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R308       22R                BottomLayer R0603                    1322.440      3117.717      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R307       22R                BottomLayer R0603                    1456.300      3117.717      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R306       22R                BottomLayer R0603                    1590.158      3117.717      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R305       22R                BottomLayer R0603                    822.440       2705.906      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R304       22R                BottomLayer R0603                    956.300       2705.906      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R303       22R                BottomLayer R0603                    1090.158      2705.906      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R302       22R                BottomLayer R0603                    1322.440      2705.906      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R301       22R                BottomLayer R0603                    1456.300      2705.906      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
R300       22R                BottomLayer R0603                    1590.158      2705.906      90       SMD Chip Resistor, Thick Film, 22 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series       
P400       BRAKE_OUT          TopLayer    TH_HDR_1X2               1732.676      314.960       360      Header, 2-Pin                                                                                    
P303       REF_SW             TopLayer    TH_HDR_1X5               832.678       3255.906      180      Header, 5-Pin                                                                                    
P302       HALL               TopLayer    TH_HDR_1X5               1332.678      3255.906      180      Header, 5-Pin                                                                                    
P301       ENC2               TopLayer    TH_HDR_1X5               832.678       2844.094      180      Header, 5-Pin                                                                                    
P300       ENC1               TopLayer    TH_HDR_1X5               1332.678      2844.094      180      Header, 5-Pin                                                                                    
IC600      LD1117S33CTR       TopLayer    SOT230P700X180-4N        353.858       2954.410      90       Fixed LDO Voltage Regulator, 4.75V to 15V, 1.1V Dropout, 3.3Vout, 950mAout, SOT-223-4            
IC303      SN74LVC3G17DCUR    BottomLayer TSSOP50P310X90-8L        822.441       2952.363      180      Triple Schmitt-Trigger Buffer, 74LVC3G17, 1.65 V to 5.5 V, VSSOP-8                               
IC302      SN74LVC3G17DCUR    BottomLayer TSSOP50P310X90-8L        1322.441      2952.363      180      Triple Schmitt-Trigger Buffer, 74LVC3G17, 1.65 V to 5.5 V, VSSOP-8                               
IC301      SN74LVC3G17DCUR    BottomLayer TSSOP50P310X90-8L        822.441       2540.552      180      Triple Schmitt-Trigger Buffer, 74LVC3G17, 1.65 V to 5.5 V, VSSOP-8                               
IC300      SN74LVC3G17DCUR    BottomLayer TSSOP50P310X90-8L        1322.441      2540.552      180      Triple Schmitt-Trigger Buffer, 74LVC3G17, 1.65 V to 5.5 V, VSSOP-8                               
IC201      AT25128B-SSHL-T    TopLayer    SOP127P600X175-8N        446.292       390.937       360      EEPROM, SPI, 128 Kbit, 16K x 8bit, 20 MHz, SOIC, 8 Pins                                          
D200       BAT54S             BottomLayer SOT95P237X130-3N         696.851       1671.652      180      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
C610       100nF/10V          BottomLayer C0603                    972.441       1560.516      90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C608       100nF/10V          BottomLayer C0603                    1173.228      1883.351      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C607       100nF/10V          BottomLayer C0603                    1051.181      1883.351      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C606       100nF/10V          BottomLayer C0603                    1151.417      1473.902      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C605       100nF/10V          BottomLayer C0603                    972.677       1681.339      90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C604       100nF/10V          BottomLayer C0603                    1033.307      1473.902      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C602       100nF/10V          BottomLayer C0603                    1192.913      1560.516      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C601       100nF/10V          BottomLayer C0603                    972.677       1801.339      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C611       100uF/6V3          TopLayer    C1210                    128.740       2877.638      90       SMD Multilayer Ceramic Capacitor, 1210 [3225 Metric], 100 µF, 6.3 V, ± 20%, X5R, GRM Series      
C609       4u7/10V            TopLayer    C0603                    132.630       3002.233      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 4.7 µF, 10 V, ± 10%, X5R, MC Series        
C501       100pF/50V/5%       TopLayer    C0603                    1437.167      1263.779      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C603       4u7/10V            TopLayer    C0603                    477.875       2755.653      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 4.7 µF, 10 V, ± 10%, X5R, MC Series        
C323       100nF/10V          BottomLayer C0603                    668.898       2960.237      0        SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C322       100nF/10V          BottomLayer C0603                    1168.898      2960.237      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C320       100nF/10V          BottomLayer C0603                    1168.898      2548.426      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C319       100pF/50V/5%       BottomLayer C0603                    1066.535      3031.102      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C318       100pF/50V/5%       BottomLayer C0603                    1566.535      3031.102      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C317       100pF/50V/5%       BottomLayer C0603                    1066.535      2619.292      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C316       100pF/50V/5%       BottomLayer C0603                    1566.535      2619.292      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C315       100pF/50V/5%       BottomLayer C0603                    932.677       3031.102      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C314       100pF/50V/5%       BottomLayer C0603                    1432.677      3031.102      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C313       100pF/50V/5%       BottomLayer C0603                    932.677       2619.292      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C312       100pF/50V/5%       BottomLayer C0603                    1432.677      2619.292      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C311       100pF/50V/5%       BottomLayer C0603                    798.819       3031.102      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C310       100pF/50V/5%       BottomLayer C0603                    1298.819      3031.102      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C309       100pF/50V/5%       BottomLayer C0603                    798.819       2619.292      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C308       100pF/50V/5%       BottomLayer C0603                    1298.819      2619.292      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C307       100nF/10V          TopLayer    C0603                    606.299       3023.228      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C306       100nF/10V          TopLayer    C0603                    1097.244      3023.229      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C305       100nF/10V          TopLayer    C0603                    596.940       2615.763      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C304       100nF/10V          TopLayer    C0603                    1097.244      2611.418      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C303       1uF/10V            BottomLayer C0603                    680.708       3117.717      90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 1 µF, 10 V, ± 10%, X5R, MC Series          
C302       1uF/10V            BottomLayer C0603                    1180.708      3117.717      90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 1 µF, 10 V, ± 10%, X5R, MC Series          
C301       1uF/10V            BottomLayer C0603                    680.708       2705.906      90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 1 µF, 10 V, ± 10%, X5R, MC Series          
C300       1uF/10V            BottomLayer C0603                    1180.708      2705.906      90       SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 1 µF, 10 V, ± 10%, X5R, MC Series          
C201       100nF/10V          TopLayer    C0603                    506.510       538.361       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
P1         Interface to UC/MC TopLayer    Interface_Connector      236.220       1673.228      90       Board-To-Board Connector, 2.54 mm, 44 Contacts, Receptacle, HLE Series, Surface Mount, 2 Rows    
P2         Interface to UC/MC TopLayer    Interface_Connector      1929.133      1673.228      90       Board-To-Board Connector, 2.54 mm, 44 Contacts, Receptacle, HLE Series, Surface Mount, 2 Rows    
C200       100nF/10V          TopLayer    C0603                    1122.322      2168.524      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
C500       1uF/10V            TopLayer    C0603                    1232.676      447.960       270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 1 µF, 10 V, ± 10%, X5R, MC Series          
C502       100pF/50V/5%       TopLayer    C0603                    1437.166      1559.056      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C503       100pF/50V/5%       TopLayer    C0603                    1417.795      756.032       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C504       100pF/50V/5%       TopLayer    C0603                    1285.906      756.032       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C505       100pF/50V/5%       TopLayer    C0603                    1154.015      756.032       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 50 V, ± 5%, C0G / NP0, MC Series   
C508       10nF               TopLayer    C0603                    1549.685      756.032       360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.01 µF, 10 V, ± 10%, X7R, MCSH Series     
C507       100pF/10V          TopLayer    C0603                    1023.227      756.032       0        SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 10 V, ± 1%, C0G / NP0, MCMT Series 
C612       47uF/10V           TopLayer    C1206                    900.901       2073.622      360      SMD Multilayer Ceramic Capacitor, 1206 [3216 Metric], 47 µF, 10 V, ± 20%, X5R, GRM Series        
C614       470nF              TopLayer    C0603                    929.102       2002.374      180      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.47 µF, 16 V, ± 10%, X5R, MC Series       
C615       4u7                BottomLayer C0603                    1192.914      1682.563      270      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 4.7 µF, 10 V, ± 10%, X5R, MC Series        
D504       BAT54S             TopLayer    SOT95P237X130-3N         889.370       850.686       0        Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
D505       BAT54S             TopLayer    SOT95P237X130-3N         1025.196      850.686       0        Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
D503       BAT54S             TopLayer    SOT95P237X130-3N         1549.685      850.687       360      Small Signal Schottky Diode, Dual Series, 30 V, 200 mA, 1 V, 600 mA, 125 °C                      
L200       30R                TopLayer    L0603                    1122.322      2105.532      360      Ferrite Bead, 30 ohm, 0603 [1608 Metric], MFB Series, 3 A, 0.04 ohm, ± 25%                       
P201       DF20F-10DP-1V(56)  TopLayer    CON,_TMC_Debug_SPI       905.323       1238.229      360      Wire-To-Board Connector, 1 mm, 10 Contacts, Header, DF20 Series, Surface Mount, 2 Rows           
P500       AENC               TopLayer    TH_HDR_1X5               1382.676      314.960       180      Header, 5-Pin                                                                                    
P502       AIN_A              TopLayer    TH_HDR_1X2               732.676       314.960       180      Header, 2-Pin                                                                                    
P501       AIN_B              TopLayer    TH_HDR_1X2               932.676       314.960       180      Header, 2-Pin                                                                                    
R200       10k                TopLayer    R0603                    1087.630      2041.891      360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R500       100R               TopLayer    R0603                    1437.167      1322.835      360      SMD Chip Resistor, Thick Film, 100 ohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series      
R507       1k                 TopLayer    R0603                    881.496       693.040       180      SMD Chip Resistor, Thick Film, 1 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 0.5%, RE Series       
R508       1k                 TopLayer    R0603                    1023.227      693.040       180      SMD Chip Resistor, Thick Film, 1 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 0.5%, RE Series       
R510       100k               TopLayer    R0603                    1643.306      724.536       270      SMD Chip Resistor, Thick Film, 100 kohm, 50 V, 0603 [1608 Metric], 100 mW, ± 1%, MCWR Series     
C600       100uF/16V          TopLayer    C1210                    479.843       2626.463      90       SMD Multilayer Ceramic Capacitor, 1210 [3225 Metric], 100 µF, 16 V, ± 20%, X5R, M Series         
C506       100pF/10V          TopLayer    C0603                    881.496       756.032       0        SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 100 pF, 10 V, ± 1%, C0G / NP0, MCMT Series 
C613       100nF              TopLayer    C0603                    929.102       1942.374      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
R405       10k                TopLayer    R0603                    1437.166      1795.275      180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R408       10k                TopLayer    R0603                    1437.165      1677.165      180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R409       10k                TopLayer    R0603                    1437.166      1381.890      360      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R410       10k                TopLayer    R0603                    1437.166      1440.945      180      SMD Chip Resistor, Thick Film, 10 kohm, 50 V, 0603 [1608 Metric], 63 mW, ± 1%, MC Series         
R505       4k                 TopLayer    R0805                    920.866       599.410       270      SMD Chip Resistor, Thick Film, 4 kohm, 150 V, 0805 [2012 Metric], 125 mW, ± 1%, CRCW Series      
R506       4k                 TopLayer    R0805                    1059.448      599.410       270      SMD Chip Resistor, Thick Film, 4 kohm, 150 V, 0805 [2012 Metric], 125 mW, ± 1%, CRCW Series      
C321       100nF/10V          BottomLayer C0603                    671.450       2548.426      360      SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.1 µF, 10 V, ± 10%, X7R, MC Series        
XTL200     25MHz              TopLayer    FOX924B-25.000           1092.677      2282.339      180      TCXO, 25 MHz, 2.5 ppm, SMD, 5mm x 3.2mm, HCMOS, 3.3 V, FOX924 Series                             
