v1.0 ------ 16.01.2020:	‣ First release.
v1.1 rc1 -- 08.06.2020:	‣ Removed pinheader J103.
    					‣ Replaced 2x M4 SMT screw connections J101 and J102 with Phoenix Contact 2pin, 1902547 J101.
    					‣ Replaced 3x M4 SMT screw connections J104, J105 and J106 with Phoenix Contact 3pin, 1904150 J102.
    					‣ Pin assignment reversed: +5V, GND, HALL_U, HALL-V, HALL-W → HALL-W, HALL-V, HALL-U, GND, +5V.
						‣ DIAG signal removed from DIO1 (J201).
    					‣ Added C129.
    					‣ Added testpoint for switching regulator output.
v1.1 ------	28.08.2020:	‣ Removed empty track from layout.