Summary Drawing Report
C:/tmp/20_057283f/worklib/02_057283e_top/physical/08_057283e.brd
Sat Dec 11 16:32:50 2021

Drawing Statistics:
    Drawing Extents  XL(-10875.00)  YL(-9610.00)  XU(25125.00)  YU(14390.00)
    Dimensions in mils with 2 decimal places
    Layers:  Total(6)  Routing(5)  Planes(1)
    Design Thickness: 53.400000 mils
    Package Symbols:  Total(147)  Mirrored(38)  Embedded(0)  Pins(416)
    Mechanical Symbols:  Total(17)  Mirrored(3)  Pins(6)
    Format Symbols:  Total(8)
    DRC State: UP TO DATE
    DRC Errors: 0
    Short DRC: 0
    Waived DRC: 0
    Padstack Definitions: 213
    Dynamic shapes:  Total(16)  Out_of_date(0)
    Functions:   Assigned(151)  Unassigned(0)  Total(151)
    Poly Via (pVia) Sites:  0

Drilling Statistics:
    Minimum Drill Size (in):  0.008000
    Drills:  Total(753)  Standard NC(753)  Nonstandard(0)
    Holes:  Plated(751)  Non-Plated(2)
    MultiDrill Padstacks:  0
    Vias:  Thru(644)  BBVias(0)  Microvia(0)  HDI(0)

Connection Statistics:
    Connections:  W/Rats(290)  No/Rats(0)  Total(290)
    Already Connected:  W/Rats(290)  No/Rats(0)  Total(290)
    Missing Connections: W/Rats(0)  No/Rats(0)  Total(0)
    Dangling Connections (See logfile):  1
    Connection Completion:  W/Rats(100.00%)  No/Rats(0.00%)  Total(100.00%)  
    Manh Distance (inches):  65.45
    Trace Length (inches):  W/Rats(86.85)  No/Rats(0.00)  Total(86.85)
    Number of Vias:  W/Rats(644)  No/Rats(0)  Total(644)
    Vias per Connection:  W/Rats(2.22)  No/Rats(0.00)Total(2.22)
    SMD pins with attached clines:  222

Layout Statistics:
    Components:  Placed(147)  Unplaced(0)  Total(147)
    Component Classes:  IC(12)  IO(38)  Discrete(97)  Mechanical(0)  Other(0)
    Nets: W/Rats(89)  No/Rats(0)  Total(89)
    Pins: W/Rats(379)  No/Rats(0)  Unused(35)  Unplaced(0)  Total(414)
    Equivalent ICs (1 pin = 1/14 EIC):  29
    RatTs:  0
    Router Keepin (in):   (-0.2100,-0.2100) by (4.1100,2.0700)
    Layout area (sq in):  9.85
    Average ratlength (in):   0.3
    Rat density (in/sq in):  6.645
    Double-sided rat density (in/sq in):  3.323

Layout/Pin Density Statistics
Layer,Layout Area<BR>(sq in),Components,Pins,Layout Density<BR>(sq in/EIC),Pin Density<BR>(pins/sq in)
External(Double-Sided),19.70,147,416,0.663,21.118
Embedded(0),0.00,0,0,0.000,0.000
Design,9.85,147,416,0.331,42.235

Trace Layer Statistics:
Layer,Clines/Carcs,Shapes(voids),Rectangles,Lines/Arcs,Text,Components(Pins)
TOP,266,18(81),0,0,0,109(334)
L2_GND,102,1(122),0,0,0,0(0)
L3_VCC,99,3(116),0,0,0,0(0)
L4_SIGNAL,117,3(83),0,0,0,0(0)
L5_GND,102,1(122),0,0,0,0(0)
BOTTOM,225,2(91),0,0,0,38(82)

Trace Width By Layer:
Layer,Widths (mils)
TOP,4.00 8.00 10.00 11.00 12.00 14.00 16.00 18.00 20.00 22.00 24.00 26.00 
L2_GND,
L3_VCC,
L4_SIGNAL,8.00 10.00 
L5_GND,
BOTTOM,6.00 8.00 10.00 12.00 18.00 20.00 24.00 

