Design Name G:/PROJECTS/MAX14690/revA/worklib/max14690_evkit_a/physical/max14690_evkit_a.brd
Date Fri Nov 18 14:30:04 2016
Drawing Statistics:
Drawing Extents XL(-48155.00) YL(-47945.00) XU(45135.16) YU(45827.00)
Dimensions in mils with 2 decimal places
Layers: Total(4) Routing(4) Planes(0)
Design Thickness: 36.600000 mil
Package Symbols: Total(25) Mirrored(6) Embedded(0) Pins(109)
Mechanical Symbols: Total(2) Mirrored(0) Pins(0)
Format Symbols: Total(2)
DRC State: UP TO DATE
DRC Errors: 0
Short DRC: 0
Waived DRC: 0
Padstack Definitions: 13
Dynamic shapes: Total(8) Out_of_date(0)
Functions: Assigned(26) Unassigned(0) Total(26)

Drilling Statistics:
Minimum Drill Size (in): 0.006000
Drills: Total(66) Standard NC(66) Nonstandard(0)
Holes: Plated(66) Non-Plated(0)
MultiDrill Padstacks: 0
Vias: Thru(34) BBVias(0) HDI(0)

Connection Statistics:
Connections: W/Rats(76) No/Rats(0) Total(76)
Already Connected: W/Rats(76) No/Rats(0) Total(76)
Missing Connections: W/Rats(0) No/Rats(0) Total(0)
Dangling Connections (See logfile): 0
Connection Completion: W/Rats(100.00%) No/Rats(0.00%) Total(100.00%)
Manh Distance (inches): 25.61
Trace Length (inches): W/Rats(19.42) No/Rats(0.00) Total(19.42)
Number of Vias: W/Rats(34) No/Rats(0) Total(34)
Vias per Connection: W/Rats(0.45) No/Rats(0.00)Total(0.45)
SMD pins with attached clines: 75

Layout Statistics:
Components: Placed(26) Unplaced(0) Total(26)
Component Classes: IC(1) IO(7) Discrete(17) Mechanical(1) Other(0)
Nets: W/Rats(29) No/Rats(0) Total(29)
Pins: W/Rats(105) No/Rats(0) Unused(4) Unplaced(0) Total(109)
Equivalent ICs (1 pin = 1/14 EIC): 7
RatTs: 0
Router Keepin (in): (0.0150,-0.0350) by (1.1850,1.3350)
Layout area (sq in): 1.60
Average ratlength (in): 0.3
Rat density (in/sq in): 15.980
Double-sided rat density (in/sq in): 7.990

Layout/Pin Density Statistics
Layer | Layout Area (sq in) | Components | Pins | Layout Density (sq in/EIC) | Pin Density (pins/sq in)
External(Double-Sided) | 3.21 | 25 | 109 | 0.412 | 34.001
Embedded(0) | 0.00 | 0 | 0 | 0.000 | 0.000
Design | 1.60 | 25 | 109 | 0.206 | 68.002

Trace Layer Statistics:

Layer | Clines/Carcs | Shapes(voids) | Rectangles | Lines/Arcs | Text | Components(Pins)
TOP | 77 | 1(0) | 0 | 0 | 0 | 19(74)
LAYER2 | 0 | 1(47) | 0 | 0 | 0 | 0(0)
LAYER3 | 0 | 5(42) | 0 | 0 | 0 | 0(0)
BOTTOM | 12 | 1(0) | 0 | 0 | 0 | 6(35)

Trace Widths By Layer:

Layer | Widths (mils)
TOP | 2.50 5.00 8.00 10.00 20.00 30.00
LAYER2 |
LAYER3 |
BOTTOM | 5.00 8.00 10.00 20.00