(---------------------------------------------------------------------)
(                                                                     )
(    Dangling Line, Via and Antenna Report                            )
(                                                                     )
(    Drawing          : max14690_evkit_a.brd                          )
(    Software Version : 17.2P028                                      )
(    Date/Time        : Fri Nov 18 09:33:01 2016                      )
(                                                                     )
(---------------------------------------------------------------------)


Report methodology:
  - Dangling lines have at least one end not connected.
  - Dangling vias have one or no connection
      - Plus are not a test, thieving or netshort property via.
  - Antenna vias do not have connections on their start and end layers.
      - Plus they are not a thieving vias.
      - Optionally, VOLTAGE nets, testvias and through vias can be suppressed with
        the environment variable report_antennavia.
      - Section may be suppressed by variable report_noantennavia.
  - Not part of the current partition.
  - To suppress items in dangle report add the OK_DANGLE property to the via
    or connect line.



<< Antenna Vias >>
  Net                  Padstack               Location            Layers
  ---------------------------------------------------------------------------
  UNNAMED_1_CAPNP_I31_2 V30H18               (380.00 702.00)  TOP/BOTTOM 
  SYS                  V20H10               (600.00 665.00)  TOP/BOTTOM 
  SUPPLY_0             V18H8                (536.00 744.00)  TOP/BOTTOM 
  SUPPLY_0             V18H8                (662.00 738.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (955.00 546.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (655.00 550.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (600.00 535.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (545.00 550.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (806.00 789.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (730.00 990.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (690.00 990.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (650.00 990.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (610.00 990.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (559.00 989.00)  TOP/BOTTOM 
  SUPPLY_0             V20H10               (519.00 989.00)  TOP/BOTTOM 
  CHGIN                V20H10               (559.00 666.00)  TOP/BOTTOM 
  BAT                  V20H10               (647.00 664.00)  TOP/BOTTOM 

<< Summary >>
  Total dangling lines:       0
  Total dangling vias:        0
  Total antenna vias:        17
