Intentional Short:

PGND and SGND nets are intentionally shorted on Bottom layer using copper shape.

