|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **QTY** | **REFERENCE** | **PART DESCRIPTION** | **MANUFACTURER** | **PART NUMBER** |
| 1 | 1 | PCB | PCB | ANALOG DEVICES | 08\_051390b |
| 2 | 4 | C1, C2,C3,C4 | CAP CER 10uF 50V X7R 2220 (Note ) | AVX CORPORATION | 22205C106KAT2A |
| 3 | 2 | C11, C12 | CAP CER 10UF 50V X5R 1206 | SAMSUNG | CL31A106MBHNNNE |
| 4 | 1 | INPUT | CONN MALE 3POS 2.54MM PITCH R/A | SULLINS | PBC03SBAN |
| 5 | 4 | L1,L2,L3,L4 | RES 0-OHM 1% PRECISION THICK FILM SMD 1206 | PANASONIC | ERJ-8GEY0R00V |
| 6 | 1 | LED1 | LED BI-COLOR GREEN/RED | LITE-ON | LTST-C235KGKRKT |
| 7 | 2 | OUTPUT1,  OUTPUT2 | CONN FEMALE 3POS 2.54MM PITCH R/A | SULLINS | PPPC031LGBN-RC |
| 8 | 1 | R1 | RES TBD THICK FILM 0805 (Note) | TBD | TBD0 |