|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **QTY** | **REFERENCE** | **PART DESCRIPTION** | **MANUFACTURER** | **PART NUMBER** |
| 1 | 1 | PCB | PCB | ANALOG DEVICES | 08\_051911b |
| 23 | 1 | C1 | CAP TBD CER 1206 (Note ) | TBD | TBD |
| 4 | 1 | C2 | CAP TBD CER 0805 (Note ) | TBD | TBD |
| 5 | 2 | J1,J2 | CONN-PCB BANANA JACK | KEYSTONE ELECTRONICS | 575-4 |
| 6 | 1 | LED1 | LED BI-COLOR GREEN/RED | LITE-ON TECHNOLOGY | LTST-C235KGKRKT |
| 7 | 1 | P1 | CONN MALE 3POS 2.54MM PITCH R/A | SULLINS | PBC03SBAN |
| 8 | 1 | R1 | RES TBD THICK FILM 0805 (Note ) | TBD | TBD |
| 9 | 1 | SMA1 | CONN-PCB STRAIGHT SMA PCB DIE CAST | TE CONNECTIVITY LTD | 5-1814832-1 |
| 10 | 1 | TP1 | CONN-PCB TEST POINT RED | KEYSTONE ELECTRONICS | 5010 |
| 11 | 1 | TP2 | CONN-PCB TEST POINT BLACK | KEYSTONE ELECTRONICS | 501 |