<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="110.1525" y2="0" width="0" layer="20"/>
<wire x1="110.1525" y1="0" x2="110.1525" y2="60.9475" width="0" layer="20"/>
<wire x1="110.1525" y1="60.9475" x2="0" y2="60.9475" width="0" layer="20"/>
<wire x1="0" y1="60.9475" x2="0" y2="0" width="0" layer="20"/>
<text>HEATBED</text>
<text>EXT_0</text>
<text>FAN</text>
<text>HEATBED</text>
<text>MAIN</text>
<text>RESET</text>
<text>I2C</text>
<text>THERM_0</text>
<text>THERM_1</text>
<text>THERM_2</text>
<text>SERVO</text>
<text>+5V</text>
<text>GND</text>
<text>HEATBED</text>
<text>MAIN POWER</text>
<text>AUX-1</text>
<text>AUX-2</text>
<text>AUX-3</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>+5V</text>
<text>TRAMS   V1.00</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>1</text>
<text>GND</text>
<text>VM</text>
</plain>
<libraries>
<library name="_TMC_TE_con">
<packages>
<package name="2PIN_1ROW_2.54_THT">
</package>
<package name="4PIN_1ROW_2.54_THT">
</package>
<package name="5PIN_1ROW_2.54_THT">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM77H">
<description>&lt;b&gt;3.3V CMOS Clock Oscillator&lt;/b&gt;&lt;p&gt;
Source: www.pletronics.com .. sm77h%203.3v.pdf</description>
</package>
</packages>
</library>
<library name="TMC5130_ARDUINO_SHIELD">
<packages>
<package name="ARDUINO_MEGA_SHIELD">
</package>
<package name="LITTLEFUSE_TR5_383_SERIES">
</package>
<package name="RIA_AKL_220_4_PINS">
</package>
<package name="RIA_AKL_220_2_PINS">
</package>
<package name="DFN3X3_8L">
</package>
<package name="TRINAMIC_LOGO_WHITE_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X18">
</package>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X4">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="Trinamic">
<packages>
<package name="QFP50P900X900X113-49N_NOFID">
</package>
</packages>
</library>
<library name="_TMC_TE_RCL">
<packages>
<package name="0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="_TMC_TE_D">
<packages>
<package name="SMB">
</package>
<package name="MICRO_SMP">
</package>
</packages>
</library>
<library name="Jochen_TRI">
<packages>
<package name="US8_DCU">
</package>
</packages>
</library>
<library name="LOGO">
<packages>
<package name="TRAMS_PRINT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="THERM0" library="_TMC_TE_con" package="2PIN_1ROW_2.54_THT" value="2PIN_1ROW">
<attribute name="NAME"/>
</element>
<element name="R1" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="THERM1" library="_TMC_TE_con" package="2PIN_1ROW_2.54_THT" value="2PIN_1ROW">
<attribute name="NAME"/>
</element>
<element name="R2" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="THERM2" library="_TMC_TE_con" package="2PIN_1ROW_2.54_THT" value="2PIN_1ROW">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTAL" library="crystal" package="SM77H" value="SM77H 16MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_0603" value="GREEN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RL2" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RL3" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHIELD" library="TMC5130_ARDUINO_SHIELD" package="ARDUINO_MEGA_SHIELD" value="ARDUINO_MEGA_SHIELD_BIG"/>
<element name="F2" library="TMC5130_ARDUINO_SHIELD" package="LITTLEFUSE_TR5_383_SERIES" value="LITTLEFUSE_TR5_383_SERIES">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="TMC5130_ARDUINO_SHIELD" package="LITTLEFUSE_TR5_383_SERIES" value="LITTLEFUSE_TR5_383_SERIES">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUX-4" library="SparkFun-Connectors" package="1X18" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUX-2" library="SparkFun-Connectors" package="AVR_ICSP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUX-1" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUX-3" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERVO" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERV_SUPPLY" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TMC5130" library="Trinamic" package="QFP50P900X900X113-49N_NOFID" value="">
<attribute name="OC_DIGIKEY" value="_"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="_TMC_TE_RCL" package="0603" value="2.2Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="_TMC_TE_RCL" package="0603" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="_TMC_TE_D" package="SMB" value="SMBJ43A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X_MOTOR" library="_TMC_TE_con" package="4PIN_1ROW_2.54_THT" value="">
<attribute name="NAME"/>
</element>
<element name="R_PD6" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_PD7" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TMC1" library="Trinamic" package="QFP50P900X900X113-49N_NOFID" value="">
<attribute name="OC_DIGIKEY" value="_"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="_TMC_TE_RCL" package="0603" value="2.2Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="_TMC_TE_RCL" package="0603" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="_TMC_TE_D" package="SMB" value="SMBJ43A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y_MOTOR" library="_TMC_TE_con" package="4PIN_1ROW_2.54_THT" value="">
<attribute name="NAME"/>
</element>
<element name="R_PD8" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_PD9" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TMC2" library="Trinamic" package="QFP50P900X900X113-49N_NOFID" value="">
<attribute name="OC_DIGIKEY" value="_"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0603" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="_TMC_TE_RCL" package="0603" value="2.2Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0603" value="C0603/470nF/16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="_TMC_TE_D" package="SMB" value="SMBJ43A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z_MOTOR_1" library="_TMC_TE_con" package="4PIN_1ROW_2.54_THT" value="">
<attribute name="NAME"/>
</element>
<element name="R_PD10" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_PD11" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TMC3" library="Trinamic" package="QFP50P900X900X113-49N_NOFID" value="">
<attribute name="OC_DIGIKEY" value="_"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R1206" value="R1206,0R15/0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="C0603" value="22nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="_TMC_TE_RCL" package="0603" value="2.2Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="_TMC_TE_RCL" package="0603" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="_TMC_TE_D" package="SMB" value="SMBJ43A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E0_MOTOR" library="_TMC_TE_con" package="4PIN_1ROW_2.54_THT" value="">
<attribute name="NAME"/>
</element>
<element name="R_PD12" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_PD13" library="rcl" package="R0603" value="100kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z_MOTOR_2" library="_TMC_TE_con" package="4PIN_1ROW_2.54_THT" value="">
<attribute name="NAME"/>
</element>
<element name="X_ENDSTOP" library="_TMC_TE_con" package="5PIN_1ROW_2.54_THT" value="5PIN_1ROWTHT">
<attribute name="NAME"/>
</element>
<element name="Y_ENDSTOP" library="_TMC_TE_con" package="5PIN_1ROW_2.54_THT" value="5PIN_1ROWTHT">
<attribute name="NAME"/>
</element>
<element name="Z_ENDSTOP" library="_TMC_TE_con" package="5PIN_1ROW_2.54_THT" value="5PIN_1ROWTHT">
<attribute name="NAME"/>
</element>
<element name="E0_ENDSTOP" library="_TMC_TE_con" package="5PIN_1ROW_2.54_THT" value="5PIN_1ROWTHT">
<attribute name="NAME"/>
</element>
<element name="MAIN_IN" library="TMC5130_ARDUINO_SHIELD" package="RIA_AKL_220_4_PINS" value="RIA_AKL_220_4_PINS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="Jochen_TRI" package="US8_DCU" value="SN74LVC3G17DCUR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HEATBED" library="TMC5130_ARDUINO_SHIELD" package="RIA_AKL_220_2_PINS" value="RIA_AKL_220_2_PINS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D_HB" library="_TMC_TE_D" package="MICRO_SMP" value="MSS1P6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="CHIPLED_0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="Jochen_TRI" package="US8_DCU" value="SN74LVC3G17DCUR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="EX_0" library="TMC5130_ARDUINO_SHIELD" package="RIA_AKL_220_2_PINS" value="RIA_AKL_220_2_PINS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D_HB1" library="_TMC_TE_D" package="MICRO_SMP" value="MSS1P6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0603" value="100Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="Jochen_TRI" package="US8_DCU" value="SN74LVC3G17DCUR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN" library="TMC5130_ARDUINO_SHIELD" package="RIA_AKL_220_2_PINS" value="RIA_AKL_220_2_PINS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D_HB2" library="_TMC_TE_D" package="MICRO_SMP" value="MSS1P6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIPLED_0603" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="TMC5130_ARDUINO_SHIELD" package="DFN3X3_8L" value="AON7508">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="E5-10,5" value="1000µ 30V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="E5-10,5" value="1000µ 30V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="TMC5130_ARDUINO_SHIELD" package="TRINAMIC_LOGO_WHITE_NOTEXT" value=""/>
<element name="U$11" library="LOGO" package="TRAMS_PRINT" value=""/>
<element name="R27" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VM0" library="_TMC_TE_con" package="2PIN_1ROW_2.54_THT" value="2PIN_1ROW">
<attribute name="NAME"/>
</element>
<element name="VM1" library="_TMC_TE_con" package="2PIN_1ROW_2.54_THT" value="2PIN_1ROW">
<attribute name="NAME"/>
</element>
<element name="R21" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0603" value="4.7kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="_TMC_TE_RCL" package="0603" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="TMC5130_ARDUINO_SHIELD" package="DFN3X3_8L" value="AON7508">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="TMC5130_ARDUINO_SHIELD" package="DFN3X3_8L" value="AON7508">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="THERM0" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="THERM1" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="THERM2" pad="1"/>
<contactref element="XTAL" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="RL3" pad="1"/>
<contactref element="RL2" pad="1"/>
<contactref element="SHIELD" pad="GND@4"/>
<contactref element="SHIELD" pad="GND@0"/>
<contactref element="SHIELD" pad="GND@1"/>
<contactref element="SHIELD" pad="GND@2"/>
<contactref element="SHIELD" pad="GND@3"/>
<contactref element="SERV_SUPPLY" pad="2"/>
<contactref element="SERV_SUPPLY" pad="8"/>
<contactref element="SERV_SUPPLY" pad="6"/>
<contactref element="SERV_SUPPLY" pad="4"/>
<contactref element="AUX-3" pad="7"/>
<contactref element="AUX-2" pad="2"/>
<contactref element="AUX-1" pad="4"/>
<contactref element="AUX-1" pad="3"/>
<contactref element="AUX-4" pad="2"/>
<contactref element="I2C" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="TMC5130" pad="32"/>
<contactref element="C6" pad="2"/>
<contactref element="TMC5130" pad="6"/>
<contactref element="TMC5130" pad="31"/>
<contactref element="TMC5130" pad="36"/>
<contactref element="C9" pad="1"/>
<contactref element="TMC5130" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="TMC5130" pad="11"/>
<contactref element="C15" pad="1"/>
<contactref element="TMC5130" pad="13"/>
<contactref element="TMC5130" pad="48"/>
<contactref element="TMC5130" pad="PAD"/>
<contactref element="D2" pad="A"/>
<contactref element="TMC5130" pad="23"/>
<contactref element="R_PD6" pad="1"/>
<contactref element="R_PD7" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="TMC1" pad="32"/>
<contactref element="C4" pad="2"/>
<contactref element="TMC1" pad="6"/>
<contactref element="TMC1" pad="31"/>
<contactref element="TMC1" pad="36"/>
<contactref element="C21" pad="1"/>
<contactref element="TMC1" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="TMC1" pad="11"/>
<contactref element="C20" pad="1"/>
<contactref element="TMC1" pad="13"/>
<contactref element="TMC1" pad="48"/>
<contactref element="TMC1" pad="PAD"/>
<contactref element="D4" pad="A"/>
<contactref element="TMC1" pad="23"/>
<contactref element="R_PD8" pad="1"/>
<contactref element="R_PD9" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="TMC2" pad="32"/>
<contactref element="C23" pad="2"/>
<contactref element="TMC2" pad="6"/>
<contactref element="TMC2" pad="31"/>
<contactref element="TMC2" pad="36"/>
<contactref element="C29" pad="1"/>
<contactref element="TMC2" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="TMC2" pad="11"/>
<contactref element="C28" pad="1"/>
<contactref element="TMC2" pad="13"/>
<contactref element="TMC2" pad="48"/>
<contactref element="TMC2" pad="PAD"/>
<contactref element="D5" pad="A"/>
<contactref element="TMC2" pad="23"/>
<contactref element="R_PD10" pad="1"/>
<contactref element="R_PD11" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="TMC3" pad="32"/>
<contactref element="C31" pad="2"/>
<contactref element="TMC3" pad="6"/>
<contactref element="TMC3" pad="31"/>
<contactref element="TMC3" pad="36"/>
<contactref element="C37" pad="1"/>
<contactref element="TMC3" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="TMC3" pad="11"/>
<contactref element="C36" pad="1"/>
<contactref element="TMC3" pad="13"/>
<contactref element="TMC3" pad="48"/>
<contactref element="TMC3" pad="PAD"/>
<contactref element="D6" pad="A"/>
<contactref element="TMC3" pad="23"/>
<contactref element="R_PD12" pad="1"/>
<contactref element="R_PD13" pad="1"/>
<contactref element="X_ENDSTOP" pad="3"/>
<contactref element="Y_ENDSTOP" pad="3"/>
<contactref element="Z_ENDSTOP" pad="3"/>
<contactref element="E0_ENDSTOP" pad="3"/>
<contactref element="IC6" pad="4"/>
<contactref element="C41" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C38" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C39" pad="2"/>
<contactref element="T2" pad="S0"/>
<contactref element="T2" pad="S1"/>
<contactref element="T2" pad="S2"/>
<contactref element="C42" pad="-"/>
<contactref element="C43" pad="-"/>
<contactref element="MAIN_IN" pad="P$1"/>
<contactref element="MAIN_IN" pad="P$3"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="VM0" pad="1"/>
<contactref element="VM1" pad="1"/>
<contactref element="T3" pad="S1"/>
<contactref element="T3" pad="S0"/>
<contactref element="T3" pad="S2"/>
<contactref element="T1" pad="S1"/>
<contactref element="T1" pad="S0"/>
<contactref element="T1" pad="S2"/>
</signal>
<signal name="ENDSTOP_X_LEFT">
<contactref element="TMC5130" pad="8"/>
<contactref element="R_PD6" pad="2"/>
<contactref element="X_ENDSTOP" pad="5"/>
<contactref element="C45" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="XTAL" pad="4"/>
<contactref element="XTAL" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="SHIELD" pad="5V@0"/>
<contactref element="SHIELD" pad="5V@1"/>
<contactref element="SHIELD" pad="5V@2"/>
<contactref element="SERV_SUPPLY" pad="7"/>
<contactref element="SERV_SUPPLY" pad="1"/>
<contactref element="SERV_SUPPLY" pad="3"/>
<contactref element="SERV_SUPPLY" pad="5"/>
<contactref element="AUX-3" pad="1"/>
<contactref element="AUX-2" pad="1"/>
<contactref element="AUX-1" pad="1"/>
<contactref element="AUX-1" pad="2"/>
<contactref element="AUX-4" pad="1"/>
<contactref element="TMC5130" pad="10"/>
<contactref element="C5" pad="1"/>
<contactref element="TMC1" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="TMC2" pad="10"/>
<contactref element="C22" pad="1"/>
<contactref element="TMC3" pad="10"/>
<contactref element="C30" pad="1"/>
<contactref element="X_ENDSTOP" pad="2"/>
<contactref element="X_ENDSTOP" pad="4"/>
<contactref element="Y_ENDSTOP" pad="2"/>
<contactref element="Y_ENDSTOP" pad="4"/>
<contactref element="Z_ENDSTOP" pad="2"/>
<contactref element="Z_ENDSTOP" pad="4"/>
<contactref element="E0_ENDSTOP" pad="2"/>
<contactref element="E0_ENDSTOP" pad="4"/>
<contactref element="IC6" pad="8"/>
<contactref element="C41" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="I2C" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C38" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="C39" pad="1"/>
<contactref element="R34" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="C44" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="C49" pad="2"/>
</signal>
<signal name="ENDSTOP_X_RIGHT">
<contactref element="TMC5130" pad="9"/>
<contactref element="R_PD7" pad="2"/>
<contactref element="X_ENDSTOP" pad="1"/>
<contactref element="C44" pad="1"/>
</signal>
<signal name="ENDSTOP_Y_LEFT">
<contactref element="TMC1" pad="8"/>
<contactref element="R_PD8" pad="2"/>
<contactref element="Y_ENDSTOP" pad="5"/>
<contactref element="C47" pad="1"/>
</signal>
<signal name="ENDSTOP_Y_RIGHT">
<contactref element="TMC1" pad="9"/>
<contactref element="R_PD9" pad="2"/>
<contactref element="Y_ENDSTOP" pad="1"/>
<contactref element="C46" pad="1"/>
</signal>
<signal name="ENDSTOP_Z_LEFT">
<contactref element="TMC2" pad="8"/>
<contactref element="R_PD10" pad="2"/>
<contactref element="Z_ENDSTOP" pad="5"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="ENDSTOP_Z_RIGHT">
<contactref element="TMC2" pad="9"/>
<contactref element="R_PD11" pad="2"/>
<contactref element="Z_ENDSTOP" pad="1"/>
<contactref element="C40" pad="1"/>
</signal>
<signal name="MAIN_POWER">
<contactref element="F1" pad="P$1"/>
<contactref element="MAIN_IN" pad="P$2"/>
</signal>
<signal name="HEATBED">
<contactref element="IC6" pad="6"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="1"/>
<contactref element="SHIELD" pad="8"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="V_HEATBED">
<contactref element="LED2" pad="A"/>
<contactref element="F2" pad="P$2"/>
<contactref element="C42" pad="+"/>
<contactref element="HEATBED" pad="P$2"/>
<contactref element="D_HB" pad="C"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="VM">
<contactref element="LED3" pad="A"/>
<contactref element="F1" pad="P$2"/>
<contactref element="C7" pad="1"/>
<contactref element="TMC5130" pad="39"/>
<contactref element="C15" pad="2"/>
<contactref element="TMC5130" pad="21"/>
<contactref element="TMC5130" pad="40"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="C16" pad="1"/>
<contactref element="TMC1" pad="39"/>
<contactref element="C20" pad="2"/>
<contactref element="TMC1" pad="21"/>
<contactref element="TMC1" pad="40"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="C24" pad="1"/>
<contactref element="TMC2" pad="39"/>
<contactref element="C28" pad="2"/>
<contactref element="TMC2" pad="21"/>
<contactref element="TMC2" pad="40"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="C32" pad="1"/>
<contactref element="TMC3" pad="39"/>
<contactref element="C36" pad="2"/>
<contactref element="TMC3" pad="21"/>
<contactref element="TMC3" pad="40"/>
<contactref element="C34" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="D6" pad="C"/>
<contactref element="EX_0" pad="P$2"/>
<contactref element="D_HB1" pad="C"/>
<contactref element="FAN" pad="P$2"/>
<contactref element="D_HB2" pad="C"/>
<contactref element="C43" pad="+"/>
<contactref element="VM0" pad="2"/>
<contactref element="VM1" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="SHIELD" pad="RESET"/>
</signal>
<signal name="SCK">
<contactref element="SHIELD" pad="52"/>
<contactref element="AUX-3" pad="5"/>
<contactref element="TMC5130" pad="4"/>
<contactref element="TMC1" pad="4"/>
<contactref element="TMC2" pad="4"/>
<contactref element="TMC3" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="SHIELD" pad="50"/>
<contactref element="AUX-3" pad="3"/>
<contactref element="TMC5130" pad="7"/>
<contactref element="TMC1" pad="7"/>
<contactref element="TMC2" pad="7"/>
<contactref element="TMC3" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="SHIELD" pad="51"/>
<contactref element="AUX-3" pad="4"/>
<contactref element="TMC5130" pad="5"/>
<contactref element="TMC1" pad="5"/>
<contactref element="TMC2" pad="5"/>
<contactref element="TMC3" pad="5"/>
</signal>
<signal name="CS_X">
<contactref element="TMC5130" pad="3"/>
<contactref element="SHIELD" pad="46"/>
</signal>
<signal name="THERM0">
<contactref element="C12" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="THERM0" pad="2"/>
<contactref element="SHIELD" pad="A13"/>
</signal>
<signal name="THERM1">
<contactref element="C13" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="THERM1" pad="2"/>
<contactref element="SHIELD" pad="A14"/>
</signal>
<signal name="THERM2">
<contactref element="C14" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="THERM2" pad="2"/>
<contactref element="SHIELD" pad="A15"/>
</signal>
<signal name="HEAT_E0">
<contactref element="SHIELD" pad="10"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="DRV_EN_X">
<contactref element="SHIELD" pad="38"/>
<contactref element="TMC5130" pad="29"/>
</signal>
<signal name="CLK">
<contactref element="XTAL" pad="3"/>
<contactref element="TMC5130" pad="2"/>
<contactref element="TMC1" pad="2"/>
<contactref element="TMC2" pad="2"/>
<contactref element="TMC3" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="RL3" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$25">
<contactref element="RL2" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="CS_Y">
<contactref element="TMC1" pad="3"/>
<contactref element="SHIELD" pad="49"/>
</signal>
<signal name="CS_Z">
<contactref element="TMC2" pad="3"/>
<contactref element="SHIELD" pad="48"/>
</signal>
<signal name="CS_E0">
<contactref element="TMC3" pad="3"/>
<contactref element="SHIELD" pad="47"/>
</signal>
<signal name="DRV_EN_E0">
<contactref element="SHIELD" pad="24"/>
<contactref element="TMC3" pad="29"/>
</signal>
<signal name="DRV_EN_Y">
<contactref element="TMC1" pad="29"/>
<contactref element="SHIELD" pad="A8"/>
</signal>
<signal name="DRV_EN_Z">
<contactref element="TMC2" pad="29"/>
<contactref element="SHIELD" pad="A2"/>
</signal>
<signal name="D53">
<contactref element="SHIELD" pad="53"/>
<contactref element="AUX-3" pad="6"/>
</signal>
<signal name="A5">
<contactref element="SHIELD" pad="A5"/>
<contactref element="AUX-2" pad="3"/>
</signal>
<signal name="A10">
<contactref element="SHIELD" pad="A10"/>
<contactref element="AUX-2" pad="5"/>
</signal>
<signal name="D44">
<contactref element="SHIELD" pad="44"/>
<contactref element="AUX-2" pad="7"/>
</signal>
<signal name="A12">
<contactref element="SHIELD" pad="A12"/>
<contactref element="AUX-2" pad="9"/>
</signal>
<signal name="A11">
<contactref element="SHIELD" pad="A11"/>
<contactref element="AUX-2" pad="10"/>
</signal>
<signal name="D42">
<contactref element="SHIELD" pad="42"/>
<contactref element="AUX-2" pad="8"/>
</signal>
<signal name="D40">
<contactref element="SHIELD" pad="40"/>
<contactref element="AUX-2" pad="6"/>
</signal>
<signal name="A9">
<contactref element="SHIELD" pad="A9"/>
<contactref element="AUX-2" pad="4"/>
</signal>
<signal name="D4">
<contactref element="SHIELD" pad="4"/>
<contactref element="SERVO" pad="4"/>
</signal>
<signal name="D5">
<contactref element="SHIELD" pad="5"/>
<contactref element="SERVO" pad="3"/>
</signal>
<signal name="D6">
<contactref element="SHIELD" pad="6"/>
<contactref element="SERVO" pad="2"/>
</signal>
<signal name="D11">
<contactref element="SHIELD" pad="11"/>
<contactref element="SERVO" pad="1"/>
</signal>
<signal name="D0">
<contactref element="SHIELD" pad="0"/>
<contactref element="AUX-1" pad="8"/>
</signal>
<signal name="D1">
<contactref element="SHIELD" pad="1"/>
<contactref element="AUX-1" pad="6"/>
</signal>
<signal name="A3">
<contactref element="SHIELD" pad="A3"/>
<contactref element="AUX-1" pad="5"/>
</signal>
<signal name="A4">
<contactref element="SHIELD" pad="A4"/>
<contactref element="AUX-1" pad="7"/>
</signal>
<signal name="D16">
<contactref element="SHIELD" pad="16"/>
<contactref element="AUX-4" pad="18"/>
</signal>
<signal name="D17">
<contactref element="SHIELD" pad="17"/>
<contactref element="AUX-4" pad="17"/>
</signal>
<signal name="D23">
<contactref element="SHIELD" pad="23"/>
<contactref element="AUX-4" pad="16"/>
</signal>
<signal name="D25">
<contactref element="SHIELD" pad="25"/>
<contactref element="AUX-4" pad="15"/>
</signal>
<signal name="D27">
<contactref element="SHIELD" pad="27"/>
<contactref element="AUX-4" pad="14"/>
</signal>
<signal name="D29">
<contactref element="SHIELD" pad="29"/>
<contactref element="AUX-4" pad="13"/>
</signal>
<signal name="D31">
<contactref element="SHIELD" pad="31"/>
<contactref element="AUX-4" pad="12"/>
</signal>
<signal name="D33">
<contactref element="SHIELD" pad="33"/>
<contactref element="AUX-4" pad="11"/>
</signal>
<signal name="D35">
<contactref element="SHIELD" pad="35"/>
<contactref element="AUX-4" pad="10"/>
</signal>
<signal name="D37">
<contactref element="SHIELD" pad="37"/>
<contactref element="AUX-4" pad="9"/>
</signal>
<signal name="D41">
<contactref element="SHIELD" pad="41"/>
<contactref element="AUX-4" pad="7"/>
</signal>
<signal name="D39">
<contactref element="SHIELD" pad="39"/>
<contactref element="AUX-4" pad="8"/>
</signal>
<signal name="D43">
<contactref element="SHIELD" pad="43"/>
<contactref element="AUX-4" pad="6"/>
</signal>
<signal name="D45">
<contactref element="SHIELD" pad="45"/>
<contactref element="AUX-4" pad="5"/>
</signal>
<signal name="D32">
<contactref element="SHIELD" pad="32"/>
<contactref element="AUX-4" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="SHIELD" pad="20"/>
<contactref element="R19" pad="1"/>
<contactref element="I2C" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="SHIELD" pad="21"/>
<contactref element="I2C" pad="4"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="SENSE2">
<contactref element="R7" pad="2"/>
<contactref element="TMC5130" pad="17"/>
</signal>
<signal name="SENSE1">
<contactref element="TMC5130" pad="44"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="TMC5130" pad="37"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C8" pad="2"/>
<contactref element="TMC5130" pad="35"/>
</signal>
<signal name="N$10">
<contactref element="TMC5130" pad="38"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="TMC5130" pad="34"/>
<contactref element="R6" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="TMC5130" pad="33"/>
<contactref element="C6" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="POSPULSE">
<contactref element="TMC5130" pad="27"/>
<contactref element="TMC1" pad="27"/>
<contactref element="TMC2" pad="27"/>
<contactref element="TMC3" pad="27"/>
<contactref element="SHIELD" pad="3"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="INTERRUPT">
<contactref element="TMC5130" pad="26"/>
<contactref element="TMC1" pad="26"/>
<contactref element="TMC2" pad="26"/>
<contactref element="TMC3" pad="26"/>
<contactref element="SHIELD" pad="2"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="M1A1_X">
<contactref element="TMC5130" pad="46"/>
<contactref element="X_MOTOR" pad="1"/>
</signal>
<signal name="M1A2_X">
<contactref element="TMC5130" pad="42"/>
<contactref element="X_MOTOR" pad="2"/>
</signal>
<signal name="M1B1_X">
<contactref element="TMC5130" pad="15"/>
<contactref element="X_MOTOR" pad="3"/>
</signal>
<signal name="M1B2_X">
<contactref element="TMC5130" pad="19"/>
<contactref element="X_MOTOR" pad="4"/>
</signal>
<signal name="SENSE3">
<contactref element="R10" pad="2"/>
<contactref element="TMC1" pad="17"/>
</signal>
<signal name="SENSE4">
<contactref element="TMC1" pad="44"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="TMC1" pad="37"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C17" pad="2"/>
<contactref element="TMC1" pad="35"/>
</signal>
<signal name="N$6">
<contactref element="TMC1" pad="38"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="TMC1" pad="34"/>
<contactref element="R12" pad="2"/>
<contactref element="C21" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="TMC1" pad="33"/>
<contactref element="C4" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="M1A2_Y">
<contactref element="TMC1" pad="42"/>
<contactref element="Y_MOTOR" pad="2"/>
</signal>
<signal name="M1B1_Y">
<contactref element="TMC1" pad="15"/>
<contactref element="Y_MOTOR" pad="3"/>
</signal>
<signal name="M1B2_Y">
<contactref element="TMC1" pad="19"/>
<contactref element="Y_MOTOR" pad="4"/>
</signal>
<signal name="M1A1_Y">
<contactref element="TMC1" pad="46"/>
<contactref element="Y_MOTOR" pad="1"/>
</signal>
<signal name="SENSE5">
<contactref element="R13" pad="2"/>
<contactref element="TMC2" pad="17"/>
</signal>
<signal name="SENSE6">
<contactref element="TMC2" pad="44"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="TMC2" pad="37"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C25" pad="2"/>
<contactref element="TMC2" pad="35"/>
</signal>
<signal name="N$16">
<contactref element="TMC2" pad="38"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="TMC2" pad="34"/>
<contactref element="R15" pad="2"/>
<contactref element="C29" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="TMC2" pad="33"/>
<contactref element="C23" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="M1A1_Z">
<contactref element="TMC2" pad="46"/>
<contactref element="Z_MOTOR_1" pad="1"/>
</signal>
<signal name="M1A2_Z">
<contactref element="TMC2" pad="42"/>
<contactref element="Z_MOTOR_2" pad="2"/>
</signal>
<signal name="M1B1_Z">
<contactref element="TMC2" pad="15"/>
<contactref element="Z_MOTOR_1" pad="3"/>
</signal>
<signal name="M1B2_Z">
<contactref element="TMC2" pad="19"/>
<contactref element="Z_MOTOR_2" pad="4"/>
</signal>
<signal name="SENSE7">
<contactref element="R16" pad="2"/>
<contactref element="TMC3" pad="17"/>
</signal>
<signal name="SENSE8">
<contactref element="TMC3" pad="44"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="TMC3" pad="37"/>
<contactref element="C33" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="C33" pad="2"/>
<contactref element="TMC3" pad="35"/>
</signal>
<signal name="N$21">
<contactref element="TMC3" pad="38"/>
<contactref element="C32" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="TMC3" pad="34"/>
<contactref element="R18" pad="2"/>
<contactref element="C37" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="TMC3" pad="33"/>
<contactref element="C31" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="ENDSTOP_E0_LEFT">
<contactref element="TMC3" pad="8"/>
<contactref element="R_PD12" pad="2"/>
<contactref element="E0_ENDSTOP" pad="5"/>
<contactref element="C49" pad="1"/>
</signal>
<signal name="ENDSTOP_E0_RIGHT">
<contactref element="TMC3" pad="9"/>
<contactref element="R_PD13" pad="2"/>
<contactref element="E0_ENDSTOP" pad="1"/>
<contactref element="C48" pad="1"/>
</signal>
<signal name="M1A1_E0">
<contactref element="TMC3" pad="46"/>
<contactref element="E0_MOTOR" pad="1"/>
</signal>
<signal name="M1A2_E0">
<contactref element="TMC3" pad="42"/>
<contactref element="E0_MOTOR" pad="2"/>
</signal>
<signal name="M1B1_E0">
<contactref element="TMC3" pad="15"/>
<contactref element="E0_MOTOR" pad="3"/>
</signal>
<signal name="M1B2_E0">
<contactref element="TMC3" pad="19"/>
<contactref element="E0_MOTOR" pad="4"/>
</signal>
<signal name="FAN">
<contactref element="SHIELD" pad="9"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="1"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="HEATBED" pad="P$1"/>
<contactref element="D_HB" pad="A"/>
<contactref element="LED6" pad="C"/>
<contactref element="T1" pad="D2"/>
<contactref element="T1" pad="D4"/>
<contactref element="T1" pad="D3"/>
<contactref element="T1" pad="D6"/>
<contactref element="T1" pad="D1"/>
<contactref element="T1" pad="D0"/>
<contactref element="T1" pad="D5"/>
</signal>
<signal name="N$39">
<contactref element="R32" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="T1" pad="G"/>
</signal>
<signal name="N$42">
<contactref element="R31" pad="2"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$43">
<contactref element="R30" pad="2"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$44">
<contactref element="R32" pad="2"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="LED6" pad="A"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="EX_0" pad="P$1"/>
<contactref element="D_HB1" pad="A"/>
<contactref element="LED1" pad="C"/>
<contactref element="T3" pad="D2"/>
<contactref element="T3" pad="D4"/>
<contactref element="T3" pad="D3"/>
<contactref element="T3" pad="D6"/>
<contactref element="T3" pad="D1"/>
<contactref element="T3" pad="D0"/>
<contactref element="T3" pad="D5"/>
</signal>
<signal name="N$28">
<contactref element="R9" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="T3" pad="G"/>
</signal>
<signal name="N$29">
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$30">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$31">
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="LED1" pad="A"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="FAN" pad="P$1"/>
<contactref element="D_HB2" pad="A"/>
<contactref element="LED4" pad="C"/>
<contactref element="T2" pad="D0"/>
<contactref element="T2" pad="D1"/>
<contactref element="T2" pad="D2"/>
<contactref element="T2" pad="D3"/>
<contactref element="T2" pad="D4"/>
<contactref element="T2" pad="D5"/>
<contactref element="T2" pad="D6"/>
</signal>
<signal name="N$37">
<contactref element="R25" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="T2" pad="G"/>
</signal>
<signal name="N$40">
<contactref element="R23" pad="2"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$41">
<contactref element="R22" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$45">
<contactref element="R25" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="LED4" pad="A"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="HEATBED_POWER">
<contactref element="F2" pad="P$1"/>
<contactref element="MAIN_IN" pad="P$4"/>
</signal>
<signal name="LEER">
</signal>
<signal name="N$1">
<contactref element="Z_MOTOR_1" pad="2"/>
<contactref element="Z_MOTOR_2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="Z_MOTOR_1" pad="4"/>
<contactref element="Z_MOTOR_2" pad="3"/>
</signal>
<signal name="D36">
<contactref element="SHIELD" pad="36"/>
<contactref element="AUX-4" pad="4"/>
</signal>
<signal name="D34">
<contactref element="SHIELD" pad="34"/>
<contactref element="AUX-3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
