
Testing combination 1
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 4096
Burst size  = 0
DMA copy started
Test combination 1 passed

Cycles = 3811, Throughput = 5158.960938 MB/s


Testing combination 2
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 4096
Burst size  = 0
DMA copy started
Test combination 2 passed

Cycles = 2581, Throughput = 7617.512695 MB/s


Testing combination 3
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 4096
Burst size  = 1
DMA copy started
Test combination 3 passed

Cycles = 3194, Throughput = 6155.541504 MB/s


Testing combination 4
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 4096
Burst size  = 1
DMA copy started
Test combination 4 passed

Cycles = 2581, Throughput = 7617.512695 MB/s


Testing combination 5
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 4096
Burst size  = 2
DMA copy started
Test combination 5 passed

Cycles = 3192, Throughput = 6159.398438 MB/s


Testing combination 6
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 4096
Burst size  = 2
DMA copy started
Test combination 6 passed

Cycles = 2580, Throughput = 7620.465332 MB/s


Testing combination 7
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 4096
Burst size  = 3
DMA copy started
Test combination 7 passed

Cycles = 2890, Throughput = 6803.044922 MB/s


Testing combination 8
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 4096
Burst size  = 3
DMA copy started
Test combination 8 passed

Cycles = 2581, Throughput = 7617.512695 MB/s


Testing combination 9
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 8192
Burst size  = 0
DMA copy started
Test combination 9 passed

Cycles = 7496, Throughput = 5245.677734 MB/s


Testing combination 10
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 8192
Burst size  = 0
DMA copy started
Test combination 10 passed

Cycles = 5041, Throughput = 7800.356934 MB/s


Testing combination 11
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 8192
Burst size  = 1
DMA copy started
Test combination 11 passed

Cycles = 6267, Throughput = 6274.389648 MB/s


Testing combination 12
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 8192
Burst size  = 1
DMA copy started
Test combination 12 passed

Cycles = 5038, Throughput = 7805.001953 MB/s


Testing combination 13
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 8192
Burst size  = 2
DMA copy started
Test combination 13 passed

Cycles = 6264, Throughput = 6277.394531 MB/s


Testing combination 14
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 8192
Burst size  = 2
DMA copy started
Test combination 14 passed

Cycles = 5041, Throughput = 7800.356934 MB/s


Testing combination 15
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 8192
Burst size  = 3
DMA copy started
Test combination 15 passed

Cycles = 5655, Throughput = 6953.421875 MB/s


Testing combination 16
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 8192
Burst size  = 3
DMA copy started
Test combination 16 passed

Cycles = 5041, Throughput = 7800.356934 MB/s


Testing combination 17
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 16384
Burst size  = 0
DMA copy started
Test combination 17 passed

Cycles = 14869, Throughput = 5289.071289 MB/s


Testing combination 18
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 16384
Burst size  = 0
DMA copy started
Test combination 18 passed

Cycles = 9954, Throughput = 7900.663086 MB/s


Testing combination 19
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 16384
Burst size  = 1
DMA copy started
Test combination 19 passed

Cycles = 12412, Throughput = 6336.062012 MB/s


Testing combination 20
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 16384
Burst size  = 1
DMA copy started
Test combination 20 passed

Cycles = 9954, Throughput = 7900.663086 MB/s


Testing combination 21
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 16384
Burst size  = 2
DMA copy started
Test combination 21 passed

Cycles = 12409, Throughput = 6337.593750 MB/s


Testing combination 22
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 16384
Burst size  = 2
DMA copy started
Test combination 22 passed

Cycles = 9954, Throughput = 7900.663086 MB/s


Testing combination 23
Internal memory type = 0x0
External memory type = 0x1
Buffer count = 16384
Burst size  = 3
DMA copy started
Test combination 23 passed

Cycles = 11184, Throughput = 7031.759766 MB/s


Testing combination 24
Internal memory type = 0x1
External memory type = 0x0
Buffer count = 16384
Burst size  = 3
DMA copy started
Test combination 24 passed

Cycles = 9955, Throughput = 7899.869629 MB/s


Testing combination 25
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 4096
Burst size  = 0
DMA copy started
Test combination 25 passed

Cycles = 4331, Throughput = 4539.552246 MB/s


Testing combination 26
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 4096
Burst size  = 0
DMA copy started
Test combination 26 passed

Cycles = 5113, Throughput = 3845.257080 MB/s


Testing combination 27
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 4096
Burst size  = 1
DMA copy started
Test combination 27 passed

Cycles = 3217, Throughput = 6111.532715 MB/s


Testing combination 28
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 4096
Burst size  = 1
DMA copy started
Test combination 28 passed

Cycles = 4861, Throughput = 4044.599854 MB/s


Testing combination 29
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 4096
Burst size  = 2
DMA copy started
Test combination 29 passed

Cycles = 2911, Throughput = 6753.967773 MB/s


Testing combination 30
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 4096
Burst size  = 2
DMA copy started
Test combination 30 passed

Cycles = 4252, Throughput = 4623.894531 MB/s


Testing combination 31
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 4096
Burst size  = 3
DMA copy started
Test combination 31 passed

Cycles = 2757, Throughput = 7131.229492 MB/s


Testing combination 32
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 4096
Burst size  = 3
DMA copy started
Test combination 32 passed

Cycles = 4375, Throughput = 4493.896973 MB/s


Testing combination 33
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 8192
Burst size  = 0
DMA copy started
Test combination 33 passed

Cycles = 7548, Throughput = 5209.539063 MB/s


Testing combination 34
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 8192
Burst size  = 0
DMA copy started
Test combination 34 passed

Cycles = 10029, Throughput = 3920.789795 MB/s


Testing combination 35
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 8192
Burst size  = 1
DMA copy started
Test combination 35 passed

Cycles = 6288, Throughput = 6253.435059 MB/s


Testing combination 36
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 8192
Burst size  = 1
DMA copy started
Test combination 36 passed

Cycles = 9632, Throughput = 4082.392090 MB/s


Testing combination 37
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 8192
Burst size  = 2
DMA copy started
Test combination 37 passed

Cycles = 5674, Throughput = 6930.137695 MB/s


Testing combination 38
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 8192
Burst size  = 2
DMA copy started
Test combination 38 passed

Cycles = 8974, Throughput = 4381.725098 MB/s


Testing combination 39
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 8192
Burst size  = 3
DMA copy started
Test combination 39 passed

Cycles = 5391, Throughput = 7293.934570 MB/s


Testing combination 40
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 8192
Burst size  = 3
DMA copy started
Test combination 40 passed

Cycles = 8496, Throughput = 4628.248535 MB/s


Testing combination 41
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 16384
Burst size  = 0
DMA copy started
Test combination 41 passed

Cycles = 15257, Throughput = 5154.564941 MB/s


Testing combination 42
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 16384
Burst size  = 0
DMA copy started
Test combination 42 passed

Cycles = 19734, Throughput = 3985.162598 MB/s


Testing combination 43
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 16384
Burst size  = 1
DMA copy started
Test combination 43 passed

Cycles = 12432, Throughput = 6325.868652 MB/s


Testing combination 44
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 16384
Burst size  = 1
DMA copy started
Test combination 44 passed

Cycles = 18709, Throughput = 4203.495605 MB/s


Testing combination 45
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 16384
Burst size  = 2
DMA copy started
Test combination 45 passed

Cycles = 11204, Throughput = 7019.207520 MB/s


Testing combination 46
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 16384
Burst size  = 2
DMA copy started
Test combination 46 passed

Cycles = 17628, Throughput = 4461.266113 MB/s


Testing combination 47
Internal memory type = 0x0
External memory type = 0x2
Buffer count = 16384
Burst size  = 3
DMA copy started
Test combination 47 passed

Cycles = 10654, Throughput = 7381.565430 MB/s


Testing combination 48
Internal memory type = 0x2
External memory type = 0x0
Buffer count = 16384
Burst size  = 3
DMA copy started
Test combination 48 passed

Cycles = 16708, Throughput = 4706.918945 MB/s

All done
