Description: 

EMDMA triggerout
Core1 is used to test it.

Hardware/Software requirements:

Tested on SOM

Code modification:

N/A

Test Procedure:

Selected Launch group configurations

Results Log:

T0

Throughput mdma0 = 105.969856 MB/s

Throughput mdma1 = 105.909576 MB/s

Throughput mdma2 = 209.916718 MB/s

Throughput mdma3 = 324.191711 MB/s

Throughput mdma4 = 105.920532 MB/s

Throughput mdma5 = 105.909576 MB/s

Throughput total = 957.817993 MB/s

T1

Throughput mdma0 = 209.519424 MB/s

Throughput mdma1 = 209.353439 MB/s

Throughput mdma2 = 416.112152 MB/s

Throughput mdma3 = 642.610596 MB/s

Throughput mdma4 = 209.374847 MB/s

Throughput mdma5 = 209.348083 MB/s

Throughput total = 1896.318604 MB/s


T2

Throughput mdma0 = 164.040131 MB/s

Throughput mdma1 = 82.774231 MB/s

Throughput mdma2 = 164.550858 MB/s

Throughput mdma3 = 246.479721 MB/s

Throughput mdma4 = 124.400169 MB/s

Throughput mdma5 = 82.756668 MB/s

Throughput total = 865.001770 MB/s

T3

Throughput mdma0 = 124.307671 MB/s

Throughput mdma1 = 163.317383 MB/s

Throughput mdma2 = 82.748314 MB/s

Throughput mdma3 = 164.346191 MB/s

Throughput mdma4 = 163.206757 MB/s

Throughput mdma5 = 163.226273 MB/s

Throughput total = 861.152649 MB/s


T4

Throughput mdma0 = 82.747475 MB/s

Throughput mdma1 = 62.279053 MB/s

Throughput mdma2 = 247.574722 MB/s

Throughput mdma3 = 325.881134 MB/s

Throughput mdma4 = 82.799332 MB/s

Throughput mdma5 = 62.261539 MB/s

Throughput total = 863.543274 MB/s